Abort Conn
    When this function is selected an additional screen is presented to the
    user to prompt for the connection handle.  A response should be provided
    to the user before returning to the main menu screen.

Active Status
   When this function is selected an additional screen is presented to the
   user to prompt for a connection index or a range of indices.  Status
   information will be returned for each specified Active connection and
    does not include any information about queued ULP transactions.

Full Status
  This status reports all the information of the Active Status request
  plus information on recently closed connections.  Status information will
  be returned for each specified Active connection and does not include any
  information about queued ULP transactions.

Update Conn
  When this function is selected an additional screen is presented to the
  user to prompt for the new maximum number of connections.  Note that this
  number does not cause any active connections to be aborted.

Log Transfer
 When this function is selected and GO is pressed, the current Log file
 will be Closed, and a new Log File will be Opened.

Trace Transfer
  When this function is selected an additional screen is presented to the
  user to prompt for the Trace and verbose to be ONOFF.  the current Trace
  file will be Closed, and a new Trace file will be Opened if Trace ON is
  selected.

		End of help. Press any key to continue.......
