'
Rename
[sys]<sys>*QueueCmds.sub [sys]<sys>*TapeCmds.sub 
[sys]<sys>Save>*QueueCmds.sub [sys]<sys>Save>*TapeCmds.sub 
yesRename
[sys]<sys>*MasterCmds.sub
[sys]<sys>Save>*MasterCmds.sub
yesRename
[sys]<sys>*ClusterCmds.sub
[sys]<sys>Save>*ClusterCmds.sub
yesRename
[sys]<sys>*MakeCmd.sub
[sys]<sys>Save>*MakeCmd.sub
yesLInstall
@[f0]<sys>HdInstall.fls
[f0]<sys>
[sys]<sys>

yes
no
no
yesCopy
[kbd]
[scr]<$>.tmp
y[sys]<sys>MakeCmd?sub [sys]<sys>QueueCmds?sub [sys]<sys>LocalTapeCmds?sub [sys]<sys>MasterTapeCmds?sub [sys]<sys>MCmds?sub [sys]<sys>MasterCmds?sub [sys]<sys>ClusterCmds?subsubmit
@[scr]<$>.tmpDelete
@[scr]<$>.tmpType
[kbd]PF
Remove the diskette from the floppy drive [f0] and insert the
Standard Software Distribution diskette 2 of 7.


INSERT DISK 2:  AM                    Press  GO  when Ready                    
1AAEF
LInstall








'Standard Software Diskette 2 of 7'LInstall
@[f0]<sys>HdInstall.fls
[f0]<sys>
[sys]<sys>

yes
no
no
yesType
[kbd]
PF
Remove the diskette from the floppy drive [f0] and insert the
Standard Software Distribution diskette 3 of 7.


INSERT DISK 3:  AM                    Press  GO  when Ready                    
1AAEF
LInstall








'Standard Software Diskette 3 of 7'LInstall
@[f0]<sys>HdInstall.fls
[f0]<sys>
[sys]<sys>

yes
no
no
yesLInstall
@[f0]<sys>HdInstallConfig.fls
[f0]<sys>
[sys]<sys>

no
no
yes
yes
Type
[kbd]PF
Remove the diskette from the floppy drive [f0] and insert the
Standard Software Distribution diskette 4 of 7.


INSERT DISK 4:  AM                    Press  GO  when Ready                    
1AAEF
LInstall








'Standard Software Diskette 4 of 7'LInstall
@[f0]<sys>HdInstall.fls
[f0]<sys>
[sys]<sys>

yes
no
no
yesType
[kbd]PF
Remove the diskette from the floppy drive [f0] and insert the
Standard Software Distribution diskette 5 of 7.


INSERT DISK 5:  AM                    Press  GO  when Ready                    
1AAEF
LInstall








'Standard Software Diskette 5 of 7'LInstall
@[f0]<sys>HdInstall.fls
[f0]<sys>
[sys]<sys>

yes
no
no
yesType
[kbd]PF
Remove the diskette from the floppy drive [f0] and insert the
Standard Software Distribution diskette 6 of 7.


INSERT DISK 6:  AM                    Press  GO  when Ready                    
1AAEF
LInstall








'Standard Software Diskette 6 of 7'LInstall
@[f0]<sys>HdInstall.fls
[f0]<sys>
[sys]<sys>

yes
no
no
yesType
[kbd]PF
Remove the diskette from the floppy drive [f0] and insert the
Standard Software Distribution diskette 7 of 7.


INSERT DISK 7:  AM                    Press  GO  when Ready                    
1AAEF
LInstall








'Standard Software Diskette 7 of 7'LInstall
@[f0]<sys>HdInstall.fls
[f0]<sys>
[sys]<sys>

yes
no
no
yes	PITvB[|9,>bzYj:j?jjjjj(j0j;jSjXjjSj)7>5]'1h	3H=