
		AFSPECIAL FUNCTION KEYS  TTY and VT100 TERMINAL MODESAA

F1			Display main menu of Telnet commands

F10			Transmit TELNET Break Command

Help			Help menu

Finish			Quit Telnet (only when connection is closed)

Cancel			Cancel a command (when in command mode)
			Send Bell signal (when in TTY  data transfer mode)
			Transmits ESCAPE code (when in VT100 data transfer mode)

CodeBackspace		Transmit TELNET Backspace and Erase character Command

CodeDelete		Transmit TELNET Erase line Command

		AFSPECIAL FUNCTION KEYS  TTY TERMINAL MODEAA


Cancel			Transmit Bell signal

Return			Transmit message (with CRLF)	

CodeReturn		Carriage Return (without Line Feed)

Down Arrow		Line Feed (without Carriage Return)

Backspace		Backspace without erasing character

Delete			Erase line

Up Arrow		Vertical Tab

Tab			Horizontal Tab

Next Page		Move to the top of the next page


			AFVT100 SPECIAL FUNCTION KEYSAA

CODE BACKSPACE  Transmits the TELNET 'Delete Char' command to the host
CODE DELETE     Transmits the TELNET 'Delete Line' command to the host

COPY            Closes the PrinterRecording File
SHIFT COPY      Starts PrintingRecording (must have first used F1 P command)
CODE COPY       PrintsRecords the Screen (must have first used F1 P command)

CODESHIFTA*   Sets TELNET VT100 into 'Single Shot Mode'
  ( MUST be used in conjunction with the 'Display Escape Sequence' function )
CODESHIFTE*   Toggle the 'Display Escape Sequence' function
CODESHIFTL*   Toggle Local Mode
CODESHIFTP    Upload a text file to the host
CODESHIFTS    Toggle the 'Display Status Line' function
CODESHIFTK*   Toggle the 'Display Keystroke' function
CODESHIFT[    Standard 24 line VT100 screen
CODESHIFT]    Extended 33 line VT100 screen (VG004 hardware only)

    ** These functions are only enabled by the VT100 Test Mode=y 
       (parameter 3 on the Telnet Command Form).
       
MARK            Toggle the keyboard 'Keypad Mode'
BOUND           Toggle the terminal between 'VT100 Mode'  'TTY Mode'

			AFVT100 SPECIAL KEYSAA


CANCEL		Transmits ESCAPE code
SHIFTF1   	Transmits VT100 PF1 Key
SHIFTF2   	Transmits VT100 PF2 Key
SHIFTF3   	Transmits VT100 PF3 Key
SHIFTF4   	Transmits VT100 PF4 Key

	
			AFTELNET COMMANDSAA

Abort			Abort an opening or established connection.	

Abort output		Send AbortOutput Telnet command to remote host.

Are you there		Send AreYouThere Telnet command to remote host.

Call			Issue an active open to a remote host.

Do			Send Telnet DO command with an option.
 
Don't			Send Telnet DON'T command with an option.

Extended Options        Negotiate extended options.

Hang Up			Close an established connection.

Host Names              Display host names.

Host Status             Display host names and Status.

Interrupt Process	Send InterruptProcess Telnet command to remote host.

Listen			Issue a passive open on a local port.

Ping			Interrogate an Ethernetconnected remote host.

PrintFilename		Specify name of file or print Queue,
			 for use in VT100 Mode only.
			 (Use COPY, SHIFTCOPY  CODECOPY to control printing)

Record			Open a file for recording (TTY mode only).

Stop Record		Close the recording file (TTY mode only).

Status			Obtain connection status.

Synch			Send Synch signal to remote host.

Upload Filename		Specify a source filename for the Upload,
			 for use in VT100 Mode only.
			 (Use CODESHIFTP to perform upload)

Verbose			Turn the option negotiations display onoff.

Will			Send Telnet WILL command with an option.

Won't			Send Telnet WON'T command with an option.
                                                                               
                                                                               
End of Help. Press any key to continue.                                        
                                                                               
                                                                               
                                                                               
                               
