'  CmdPipeDrivers.sub (for Pipe Drivers)
'  param  0: sys or sys  (master or workstation installation)
'
Copy
[kbd]
[Scr]<$>args.Tmp
Yes
  'Input File'  'Output File'  '[New Line Map Mode (binary, CR, or CRLF)]'  '[Expand Tab Size (8)]'  '[Characters per line (85)]'  '[Font Device Type (Simple)]'  '[Device Setup]'  '[Page Width and Length (8.5 11)]'  '[Top and Bottom Borders (0 0)]'  '[Left and Right Borders (0 0)]'  '[Storage Allocation1K units (4)]'
Copy
[kbd]
[Scr]<$>desc.Tmp
Yes
'Convert GPAM to Draft Output'
New Command
'Pipe Simple'
[Sys]<Gps>LptSimplePipe.run
@[Scr]<$>args.Tmp
@[Scr]<$>desc.Tmp
Yes
'\0\0'
[0]<Sys>sys.cmds'
'
Copy
[kbd]
[Scr]<$>args.Tmp
Yes
  'Input File'  'Output File'  '[New Line Map Mode (binary, CR, or CRLF)]'  '[Expand Tab Size (8)]'  '[Characters per line (85)]'  '[Font Device Type (Daisy)]'  '[Device Setup]'  '[Page Width and Length (8.5 11)]'  '[Top and Bottom Borders (0 0)]'  '[Left and Right Borders (0 0)]'  '[Storage Allocation1K units (4)]'
Copy
[kbd]
[Scr]<$>desc.Tmp
Yes
'Convert Gpam to Diablo630, Envision, Nec3515 or QumeSprint9'
New Command
'Pipe Daisy'
[Sys]<Gps>DaisyPipe.run
@[Scr]<$>args.Tmp
@[Scr]<$>desc.Tmp
Yes
'\0\0'
[0]<Sys>sys.cmds'
'
Copy
[kbd]
[Scr]<$>args.Tmp
Yes
  'Input File'  'Output File'  '[New Line Map Mode (binary, CR, or CRLF)]'  '[Expand Tab Size (8)]'  '[Characters per line (85)]'  '[Font Device Type (Imagen)]'  '[Device Setup]'  '[Page Width and Length (8.5 11)]'  '[Top and Bottom Borders (0 0)]'  '[Left and Right Borders (0 0)]'  '[Storage Allocation1K units (4)]'
Copy
[kbd]
[Scr]<$>desc.Tmp
Yes
'Convert Gpam to Impress (Imagen 8300)'
New Command
'Pipe Imagen'
[Sys]<Gps>Imagen8300Pipe.run
@[Scr]<$>args.Tmp
@[Scr]<$>desc.Tmp
Yes
'\0\0'
[0]<Sys>sys.cmds'
'
Copy
[kbd]
[Scr]<$>args.Tmp
Yes
  'Input File'  'Output File'  '[New Line Map Mode (binary, CR, or CRLF)]'  '[Expand Tab Size (8)]'  '[Characters per line (85)]'  '[Font Device Type (PostScript)]'  '[Device Setup]'  '[Page Width and Length (8.5 11)]'  '[Top and Bottom Borders (0 0)]'  '[Left and Right Borders (0 0)]'  '[Storage Allocation1K units (4)]'
Copy
[kbd]
[Scr]<$>desc.Tmp
Yes
'Convert Gpam to PostScript'
New Command
'Pipe PostScript'
[Sys]<Gps>PSPipe.run
@[Scr]<$>args.Tmp
@[Scr]<$>desc.Tmp
Yes
'\0\0'
[0]<Sys>sys.cmds'
'
Copy
[kbd]
[Scr]<$>args.Tmp
Yes
  'Input File'  'Output File'  '[New Line Map Mode (binary, CR, or CRLF)]'  '[Expand Tab Size (8)]'  '[Characters per line (85)]'  '[Font Device Type (HpLaserJet)]'  '[Device Setup]'  '[Page Width and Length (8.5 11)]'  '[Top and Bottom Borders (0 0)]'  '[Left and Right Borders (0 0)]'  '[Storage Allocation1K units (4)]'
Copy
[kbd]
[Scr]<$>desc.Tmp
Yes
'Convert Gpam to PCL (HP Laser Jet)'
New Command
'Pipe LaserJet'
[Sys]<Gps>HpLaserJetPipe.run
@[Scr]<$>args.Tmp
@[Scr]<$>desc.Tmp
Yes
'\0\0'
[0]<Sys>sys.cmds'
'
Copy
[kbd]
[Scr]<$>args.Tmp
Yes
  'Input File'  'Output File'  '[New Line Map Mode (binary, CR, or CRLF)]'  '[Expand Tab Size (8)]'  '[Characters per line (85)]'  '[Font Device Type (EpFx286)]'  '[Device Setup]'  '[Page Width and Length (8.5 11)]'  '[Top and Bottom Borders (0 0)]'  '[Left and Right Borders (0 0)]'  '[Storage Allocation1K units (4)]'
Copy
[kbd]
[Scr]<$>desc.Tmp
Yes
'Convert Gpam to Epson Fx286'
New Command
'Pipe Epson'
[Sys]<Gps>EpFx286Pipe.run
@[Scr]<$>args.Tmp
@[Scr]<$>desc.Tmp
Yes
'\0\0'
[0]<Sys>sys.cmds'
'
Copy
[kbd]
[Scr]<$>args.Tmp
Yes
  'Input File'  'Output File'  '[New Line Map Mode (binary, CR, or CRLF)]'  '[Expand Tab Size (8)]'  '[Characters per line (85)]'  '[Font Device Type (CT2400)]'  '[Device Setup]'  '[Page Width and Length (8.5 11)]'  '[Top and Bottom Borders (0 0)]'  '[Left and Right Borders (0 0)]'  '[Storage Allocation1K units (4)]'
Copy
[kbd]
[Scr]<$>desc.Tmp
Yes
'Convert Gpam to Convergent Dot Matrix (DPL24C)'
New Command
'Pipe CTMatrix'
[Sys]<Gps>CTMatrixPipe.run
@[Scr]<$>args.Tmp
@[Scr]<$>desc.Tmp
Yes
'\0\0'
[0]<Sys>sys.cmds'
'