****************************************************************************
*    TCPIP X25 NGI Internet to PDN address mapping configuration file     *
****************************************************************************
*																			*
*		NOTE: On the DDN network, this file is not necessary since 			*
*			  X.25 Addresses are calculated from the Internet Address.		*
*																			*
*	This file is used for mapping Internet Addresses to X.25 Addresses.		*
*	Each line must start and end with a colon (:) and a colon must be used	*
*	between the two addresses.  The address on the  left is a standard   	*
*	Internet Address.  The number on the right is the corresponding X.25    *
*	Address for that particular Internet Address.  Remember, when using 	*
*	X.25, the NetType parameter in the 'TCPIP.Params' file is a '2'.  This *
*	tells the IP Server to send all frames destined for that Internet    	*
*	Address out on the X.25 network instead of LAN.  IP then sends the frame*
*	to the Network Gateway Interface (NGI) which reads this table to find   *
*	the X.25 Address for the Internet address specified in the frame.		*
*																			*
*	The last entry can be a default value.  All Internet Address mappings	*
*	which cannot be resolved to a specific X.25 Address will use the		*
*	default.																*
*																			*
*	Note: A maximum of 20 X.25 addresses can be configured.					*
*																			*
*	HINT:  The space between the colons (:) is significant.					*
*		   Follow the examples carfully when you edit the addresses and 	*
*		   Do not put extra space between the colons.						*
****************************************************************************

:192.140.010.001: 123456789012301:  * SAMPLE HOST 1  *
:192.140.010.002: 123456789012302:  * SAMPLE HOST 2  *
:192.140.010.003: 123456789012303:  * SAMPLE HOST 3  *
:192.140.010.004: 123456789012304:  * SAMPLE HOST 4  *
:192.140.010.005: 123456789012305:  * SAMPLE HOST 5  *
:192.140.010.006: 123456789012306:  * SAMPLE HOST 6  *
:192.140.010.007: 123456789012307:  * SAMPLE HOST 7  *
:192.140.010.008: 123456789012308:  * SAMPLE HOST 8  *
:192.140.010.009: 123456789012309:  * SAMPLE HOST 9  *
:0.0.0.0:		  123456789012310:  * DEFAULT *
FH8
tFvFP6F	uNOw
^YFPP66 F	ulF	tRPG
P6F	uOF9GsH^
FG
vNFYPFP6F	u2u^SP^S