' Install.Sub <B20FM61>  MOD 010792 D. Stager
2Copy
[Kbd]
[Vid]
PF

		    
		        BTOS FORMS DESIGNER INSTALLATION   
		    

	  If this is the server station of a cluster system, then power
	  down all cluster workstations.

	  If this is a cluster workstation, then power down all other
	  workstations except this station and the server station.

			      PRESS AE<GO>AA when ready
			      1				
?2Copy
[Kbd]
[Vid]
PF

		    
		        BTOS FORMS DESIGNER INSTALLATION   
		    

	  Power down all other workstations except this station and
	  the XE520 server.

			      PRESS AE<GO>AA when ready
			      1				
Copy
[Kbd]
[Vid]
PF

	
									
	    Volume Status will display the number of unused sectors	
		 on your [Sys] volume.					
									
	    AFPRESS AE<GO>AA to invoke Volume Status, note the number of	
		 unused sectors, then AFPRESS AE<GO>AA again to continue.	
									
	
1Screen Setup

yesVolume Status
Sys1Create Directory
1Copy
[Kbd]
[Vid]
PF

	
									
	    Installing BTOS Forms Designer WITH the graphics		
		 capable Forms Editor requires approximately 952	
		 free sectors on a BTOS workstation and a minimum	
		 of 300K memory.					
									
	    Installing BTOS Forms Designer WITHOUT the graphics 	
		 capable Forms Editor requires approximately 653 free	
		 sectors on a BTOS workstation and a minimum of 300K	
		 memory.						
									
	    If this system does not have the required space or		
		 memory available AFPRESS AE<ACTION><FINISH>AA to cancel	
		 installation.						
									
	    If this system does have the required space and memory	
		 available AFPRESS AE<GO>AA to continue.			
									
	
1Copy
[Kbd]
[Vid]
PF

			       AE GRAPHICS INSTALLATION AA
	
									
	   AE 1 AA  Install graphics capable Forms Editor.			
									
	   AE 2 AA  Install standard Forms Editor.				
									
	   To install the correct Forms Editor, enter the appropriate	
		 number (1 or 2) in the [Parameters] field of		
		 the Submit command form below, then AFPRESS AE<GO>AA.	
									
	
Submit
[B20FM61]<Sys>Choice.Sub
0 1 2''?22 
yes
1Copy
[kbd]
[vid]
PF




	
									
		  Please remove the Forms Designer diskette 1		
		  and insert diskette number 2 (B20FM62).		
									
	

			      PRESS AE<GO>AA when ready
1Copy
[kbd]
[vid]PF
		      AE Forms RunTime Library INSTALLATION AA
	
									
	    To install Forms RunTime library AFPRESS AE<GO>AA.		
									
	    Otherwise, AFPRESS AE<CANCEL><GO>AA.				
	
LCopy
[B20FM62]<Unisys>Forms.Lib

1

y1LCopy
[B20FM62]<Unisys>FormsReporter.Run

1

yCopy
[kbd]
[sys]<$>Args.Temp
yes'File' '[Form]' '[Fields?]' '[Form Image?]' '[Output]'
Copy
[kbd]
[sys]<$>Desc.Temp
yes'Produce a report describing a form and its fields.'
New Command
'FReport'
1FormsReporter.Run
@[sys]<$>Args.Temp
@[sys]<$>Desc.Temp
yes

0Copy
[kbd]
[sys]<$>Desc.Temp
yes'Print a Form to the designated printer.'
New Command
'Print Form'
1FormsReporter.Run
'File' '[Form]' '[Queue Name (default = SPL)]'
@[sys]<$>Desc.Temp
yes
'01'
0Append
[B20FM62]<sys>fdSys.Version [Kbd]
2[Sys]?2[Sys]<Sys>Sys.Version Forms Designer 6.3 installed on d|*w *n *d, yyyy, at *t:0m|
Delete
[sys]<$>Args.Temp [sys]<$>Desc.Temp
Copy
[kbd]
[vid]PF
	
									
	    The second diskette contains FmrGtd.Asm, FmTabKey.Asm,     
	    and FmValProc.Asm files.  It also contains three object    
	    modules:  4.0FmChar.Obj, 4.0FmUser.obj, and 4.0FmRun1.0bj. 
	    After completion of installation, you may copy any of      
	    these files as required for configuration of Forms.Lib.    
	    AFPRESS AE<GO>AA to continue.					
									
	
1Copy
[kbd]
[vid]PF
	Please remove the Forms Designer diskette from the disk drive
	and put it and all other software diskettes in a safe place.

	If this is a cluster system, you may now resume cluster operations.
 
	AE ********************* REBOOT THE SYSTEM ********************* AA
	AE **** TO COMPLETE INSTALLATION OF CTOS FORMS DESIGNER ****     AA
PNCopy
[Kbd]
[Vid]
PF

		    
		        BTOS FORMS DESIGNER INSTALLATION   
		    

	  If this is the server station of a cluster system, then power
	  down all cluster workstations.

	  If this is a cluster workstation, then power down all other
	  workstations except this station and the server station.

			      PRESS AE<GO>AA when ready
			      1				
?2