'
Copy
[B25CBD11]<Sys>Sys.cmds
Sys.cmds
noCopy
[B25CBD11]<Sys>Sys.cmds
Sys.cmdsInitial
yesCopy
[B25CBD11]<Sys>Exec*
Exec*
yesCopy
[B25CBD11]<Sys>Submit.run
Submit.run
yesRun
[B25CBD11]<Sys>ChangeSysVol.run0|Rename
[Sys]<Sys>Sysinit.jcl
[Sys]<Sys>pre12.3.100>Sysinit.jcl
noDelete
[Sys]<Sys>Sysinit?jclDelete
[Scr]<$*>*Copy
[Sys]<Sys>Signon.txt
[Sys]<Sys>pre12.3.100>Signon.txt
noCopy
[Sys]<Sys>Nls.sys
[Sys]<Sys>pre12.3.100>Nls.sys
noCopy
[Sys]<Sys>FormatDiskConfig.sys
[Sys]<Sys>pre12.3.100>FormatDiskConfig.sys
no|Copy
[B25CBD11]<Sys>Signon.txt
[Sys]<Sys>Signon.txt
yesCopy
[B25CBD11]<Sys>Floppy.user
[Sys]<Sys>Floppy.user
yesCopy
[B25CBD11]<Sys>Tape.user
[Sys]<Sys>Tape.user
yesCreate Directory
[Sys]<SPL>

75Create Directory
[Sys]<$000>

750?0|Create File
FileMark>VGAConfig.sys




yes|Copy
[B25CBD11]<Sys>LCopy.run
LCopy.run
yesLCopy
@[B25CBD11]<Sys>Copy.fls
[B25CBD11]<Sys>


yes
no
no
yesLCopy
SignOn.txt
[B25CBD11]<Sys>SID>


yes
no
no
yesLCopy
[B25CBD11]<Sys>Request.sys



no
no
no
yes?0|LCopy
Signon.txt
[B25CBD11]<Sys>Normal>
12.3.100>

no|Move
XVTSignOn.run

Pre12.3.100>

yes
no
yes
yesCopy
Request.sys
<$000>Pre12.3.100>Request.sys
yes0|List Request Set
[B25CBD11]<Sys>Request.sys Reques?.sys
[Scr]<$>Request.lstMake Request Set
[Scr]<$>Request.lst
Request.sys|Copy
[kbd]
[vid]PF




        
                                                                       
                Remove the diskette from the floppy disk drive and     
                reinsert the boot diskette that you originally used    
                to boot the system.                                    
                                                                       
        

                             Press AE<GO>AA when ready.

1LCopy
@[B25Boot]<Sys>Copy.fls
[B25Boot]<Sys>


yes0|Copy
[kbd]
[vid]
PF

    
                                                                           
        AFPRESS AE<G0>AA if you wish to overwrite the Operating System           
        file on your hard disk (i.e. SysImage.sys) with the Operating      
        System file from the boot diskette.                                
                                                                           
                                                                           
        Otherwise, AFPRESS AE<CANCEL><GO>AA to keep the existing                
        Operating System on your hard Disk.                                
                                                                           
    
|LCopy
SysImage.sys [B25Boot]<Sys>ps_?.sys
[B25Boot]<Sys>
[Sys]<sys>

yes
no
no
yes0|1|Copy
[kbd]
[vid]PF




        
                                                                       
                Remove the diskette from the floppy drive.             
                To continue the installation, the workstation will     
                be rebooted.                                           
                                                                       
        

                            Press AE<GO>AA to reboot.

1Run
Bootstrap.run


Sysimage.sys
.

                                                                          
                              *** NOTE ***                                
                                                                          
     Your system has now been set up to enable an Installation Manager    
     session.  Installation Manager 12.3.100 and above will use the       
     database name