'
Submit
0|[f0]|?0|0|<sys>HdInstall.Sub

            aa                                                 ab
            aa The following procedure requires 1 initialized  ab
            aa diskette.                                       ab
            aa                                                 ab
            ae Press GO to continue.                           ab
            aa

1

Cr