'
Type
[kbd]PF
AF                                                             
  The proper OS is on diskette 4 of 4.                       
  Remove the diskette from floppy drive ae00[f0]AF and insert the  
  Workstation OS Kit diskette 4 of 4.                        
                                                             
AA

INSERT DISK 4:  AM                    Press  GO  when Ready                    
1AAEF
LInstall








'Workstation OS Kit Diskette 4 of 4'Submit
00[f0]<Sys>StandAlone.sub
0