'
Type
[kbd]PF
Remove the diskette from the floppy drive [f0] and insert the
Standard Software Distribution diskette 1 of 7.


INSERT DISK 1:  AM                    Press  GO  when Ready                    
1AAEF
Run
LInstall.run










'Standard Software Diskette 1 of 7'LCopy
[f0]<sys>Command.run



yes
no
no
yesCopy
  [kbd]
  [sys]<$>Args.tmp
  Yes
 'File list' '[File prefix(s) from]' '[File prefix(s) to]' '[File suffix(s)]' '[Overwrite OK?]' '[Confirm each?]' '[Continue on error?]' '[Verify copy?]' '[Diskette]'
Copy
  [kbd]
  [sys]<$>Desc.tmp
  Yes
'Install a list of files.'
New Command
  'LInstall'
  '[sys]<sys>LInstall.Run'
  @[sys]<$>Args.tmp
  @[sys]<$>Desc.tmp
  yes
Submit
[f0]<sys>CmdsUpdate.subDelete
Update*.user Remote*.usersubmit
[f0]<sys>ContinueInstall.subRename
Save>SysInit.jcl Save>Signon.txt
SysInit.jcl SignOn.txt 
yesDelete
*Request.2.sys *Request.X.sys *Request.9.sysCopy
[nul]
[scr]<$>Request.txt
y'
'
'  The following steps take care of the requestolation
'  After the first release of CTOS II, we should change
'  the following list to include [sys]<sys>Request?sys.
'  This will allow current Request files to be fixed up.
'
Copy
[kbd]
[scr]<$>rq.tmp
yRequest.?.sys MRequest.?.sys [f0]<sys>Request.sys
List Request Set
@[scr]<$>rq.tmp
[scr]<$>request.txtLinstall
Request.9.sys Request.x.sys Request.2.sys
[f0]<sys>
[sys]<sys>

yType
[kbd]PN

    The next command is the final step in the installation.
    It should complete with 0 errors, warnings are all right.
    If a you receive a message or messages saying:

The following files have overlapping and differing requests for xxxxh

    Press Finish and consult the Release Notice for Standard Software II.

    Press GO to continue.

1
Make Request Set
[scr]<$>request.txt
Request.sysDelete
[scr]<$>Request.txt [scr]<$>rq.tmpType
[kbd]
PF
            ab
            aa                                                 ab
            aa       Update of system volume complete.         ab
            aa                                                 ab
            aa

Remove the diskette from the floppy drive [f0].

If you will be using this workstation as a software development system,
insert the Software Development Utilities Diskette 1 of 2 and type 

	Install  <GO>

OTHERWISE,

       press the hardware RESET button to bootstrap your 
       workstation; and

    IF you have just completed a REMOTE installation, 

        press the master's hardware RESET button to bootstrap
        the master.


PNpp>pwppppppppppppJpppppppp'pFphppppppppp:pDpWpdpptppppRpZp{ppppppppppps8
l+Op1es