' Install.Sub <B25PAS1>  MOD 112392, L. Lyons
2Copy
[Kbd]
[Vid]
PF

		  
		       CTOS PASCAL Compiler Installation     
		  

	  If this is the server station of a cluster system, then power
	  down all cluster workstations.

	  If this is a cluster workstation, then power down all other
	  workstations except this station and the server station.

			      PRESS AE<GO>AA when ready
1Copy
[Kbd]
[Vid]
PF

	
									
	   This installation will create commands.  Before continuing,	
		ensure that the command file is not in use elsewhere.	
									
		AFPRESS AE<ACTION><FINISH>AA to cancel installation.		
									
		AFPRESS AE<GO>AA to continue.					
									
	
			    PRESS AE<GO>AA when ready
			    1				
Copy
[Kbd]
[Vid]
PF

	
									
	    Volume Status will display the number of unused sectors	
		 on your [Sys] volume.					
									
	    AFPRESS AE<GO>AA to invoke Volume Status, note the number of	
		 unused sectors, then AFPRESS AE<GO>AA again to continue.	
									
	
1Screen Setup

yesVolume Status
Sys1Copy
[Kbd]
[Vid]
PF
	
									
	   CTOS PASCAL COMPILER requires approximately 1200		
		sectors on a CTOS workstation and you will need a 	
		minimum of 400K of memory.				
									
	   If this system does not have the required space available	
		AFPRESS AE<ACTION><FINISH>AA to cancel installation.		
									
	   If this system does have the required space available	
		AFPRESS AE<GO>AA to continue.					
									
	
1?2Copy
[Kbd]
[Vid]
PF
		  
		       CTOS PASCAL Compiler Installation     
		  

	  Power down all other workstations except this station and
	  the XE server.

			      PRESS AE<GO>AA when ready
1Copy
[Kbd]
[Vid]
PF

	
									
	    Volume Status will display the number of unused sectors	
		 on your [Sys] volume.					
									
	    AFPRESS AE<GO>AA to invoke Volume Status, note the number of	
		 unused sectors, then AFPRESS AE<GO>AA again to continue.	
									
	
1Screen Setup

yesVolume Status
Sys1Copy
[Kbd]
[Vid]
PF
	
									
	   CTOS PASCAL COMPILER requires approximately 1200		
		sectors on a CTOS workstation and you will need a 	
		minimum of 400K of memory.				
									
	   If this system does not have the required space available	
		AFPRESS AE<ACTION><FINISH>AA to cancel installation.		
									
	   If this system does have the required space available	
		AFPRESS AE<GO>AA to continue.					
									
	
1Create Directory
1

200LCopy
[B25PAS1]<Unisys>*

1

yesCopy
[kbd]
[sys]<$>Args.Tmp
yes'Source File' '[Object File]' '[List File]' '[Object List File]'
New Command
'Pascal'
1PascalFe.Run
@[Sys]<$>Args.Tmp
'Invoke the Pascal Compiler.'
y

0Copy
[kbd]
[vid]
PF




	
									
		  Please remove the Pascal Compiler diskette 1 and      
		   insert diskette number 2 (B25PAS2).                 
									
	

			      PRESS AE<GO>AA when ready
1Copy
[Kbd]
[Vid]
PF
	
									
	  Installation of CTOS PASCAL Compiler software requires	
	     [Sys]<Sys>Linker.Run with release level 12.2.0 or 	
	     greater.  AFPRESS AE<GO>AA to overwrite any existing		
	     version of [Sys]<Sys>Linker.Run.  AFPRESS AE<CANCEL><GO>AA	
	     to continue installation.					
									
	
LCopy
Linker.Run
[B25PAS2]<Unisys>
2[Sys]?2[Sys]<Sys>

yes1LCopy
[B25PAS2]<Unisys>Pascal.lib

1

yesDelete
[Sys]<$*>Args.Tmp
Append
[f0]<Sys>fdSys.Version [Kbd]
2[Sys]?2[Sys]<Sys>Sys.Version PASCAL Compiler installed on d|*w *n *d, yyyy, at *t:0m|
Copy
[kbd]
[vid]PF


	AE ***** INSTALLATION OF CTOS PASCAL COMPILER COMPLETE ***** AA


	Please remove the PASCAL Compiler disk from the disk drive and
	put it and all other diskettes in a safe place.

	If this is a cluster system, you may now resume cluster operations.

PN
PathDef 		= '[Sys]<sys>'
	   DefVol 		= Clien