'
Video
YesLCopy
00[f0]<CT>*

[Sys]<Sys>

yes
no
no
yesType
[kbd]PF
Remove the diskette from the floppy drive and insert the
SRP Utilities diskette 3 of 3.


INSERT DISK 3:  AM                    Press  GO  when Ready                    
1AAEF
LInstall








'SRP Utilities Diskette 3 of 3'Submit
00[f0]<Sys>All.sub
'[Sys]<Sys>' '[Sys]<Sys>' Sys 00[f0]        command (e.g. files) and where to get the run