 Event definitions for RAF Source


:Symbol:
	RafSourceHiPen = 0x56040000				22020.0.
:End:


:Template:  Standard
	SubSystem	= RAF Source
	SubTopic	= 1800
:End:

 If running over the RS232 interface, SubSystem is RS232 Source

:Event:					RafSourceHiPen + 1
	Template	= Standard
	Component	= 1000
	Class		= Warning
	Topic		= 0x403
	Activity	= 50002
	SendWeight	= 50
	LogWeight	= 50
	Context 	= User V1 failed to logon because of V2.

:Event:					RafSourceHiPen + 2
	Template	= Standard
	Component	= 1000
	Class		= Warning
	Topic		= 0x403
	Activity	= 50006
	SendWeight	= 50
	LogWeight	= 50
	Context 	= User V1 not authorized to do file transfer at target V2.

:Event:					RafSourceHiPen + 3
	Template	= Standard
	Component	= 1000
	Class		= Warning
	Topic		= 0x403
	Activity	= 50006
	SendWeight	= 50
	LogWeight	= 50
	Context 	= User V1, monitoring inhibited, not allowed to viewcontrol Target V2.

:Event:					RafSourceHiPen + 4
	Template	= Standard
	Component	= 2000
	Class		= Fatal
	Topic		= 0x401
	Activity	= 14000007
	SendWeight	= 250
	LogWeight	= 250
	Context 	= User V1, erc $S1 encountered when opening V2.

:Event:					RafSourceHiPen + 5
	Template	= Standard
	Component	= 1000
	Class		= Fatal
	Topic		= 0x401
	Activity	= 14049999
	SendWeight	= 250
	LogWeight	= 250
	Context 	= User V1 fatal error = S1.

:Event:					RafSourceHiPen + 6
	Template	= Standard
	Component	= 4006
	Class		= Fatal
	Topic		= 0x403
	Activity	= 8000001
	SendWeight	= 250
	LogWeight	= 250
	Context 	= User V1, Modem Service failure, erc = S1.

:Event:					RafSourceHiPen + 7
	Template	= Standard
	Component	= 1004
	Class		= Fatal
	Topic		= 0x401
	Activity	= 14049999
	SendWeight	= 250
	LogWeight	= 250
	Context 	= User V1, PEM server error, erc = S1.

:Event:					RafSourceHiPen + 8
	Template	= Standard
	Component	= 3003
	Class		= Warning
	Topic		= 0x401
	Activity	= 14049999
	SendWeight	= 50
	LogWeight	= 50
	Context 	= User V1, MCR server error, erc = $S1.

:Event:					RafSourceHiPen + 9
	Template	= Standard
	Component	= 2999
	Class		= Warning
	Topic		= 0x401
	Activity	= 14049999
	SendWeight	= 50
	LogWeight	= 50
	Context 	= User V1, file transfer terminated with error S1 at Target V2.

:Event:					RafSourceHiPen + 10
	Template	= Standard
	Component	= 3003
	Class		= Warning
	Topic		= 0x401
	Activity	= 14049999
	SendWeight	= 50
	LogWeight	= 50
	Context 	= User V1, Erc = S1 while accessing MCR [$V2].

:Event:					RafSourceHiPen + 11
	Template	= Standard
	Component	= 1000
	Class		= Normal
	Topic		= 0x403
	Activity	= 50000
	SendWeight	= 40
	LogWeight	= 40
	Context 	= User V1 logged on.


 new ones added... Bernie

:Event:					RafSourceHiPen + 12
	Template	= Standard
	Component	= 1000
	Class		= Normal
	Topic		= 0x403
	Activity	= 50000
	SendWeight	= 250
	LogWeight	= 250
	Context 	= User V2, view session begin.

:Event:					RafSourceHiPen + 13
	Template	= Standard
	Component	= 1000
	Class		= Normal
	Topic		= 0x403
	Activity	= 50001
	SendWeight	= 250
	LogWeight	= 250
	Context 	= User V2, view session end.

:Event:					RafSourceHiPen + 14
	Template	= Standard
	Component	= 1000
	Class		= Normal
	Topic		= 0x403
	Activity	= 50000
	SendWeight	= 250
	LogWeight	= 250
	Context 	= User V2, control session begin.

:Event:					RafSourceHiPen + 15
	Template	= Standard
	Component	= 1000
	Class		= Normal
	Topic		= 0x403
	Activity	= 50001
	SendWeight	= 250
	LogWeight	= 250
	Context 	= User V2, control session end.

:Event:					RafSourceHiPen + 16
	Template	= Standard
	Component	= 1000
	Class		= Normal
	Topic		= 0x403
	Activity	= 50000
	SendWeight	= 250
	LogWeight	= 250
	Context 	= User V2, control at logon session begin.

:Event:					RafSourceHiPen + 17
	Template	= Standard
	Component	= 1000
	Class		= Normal
	Topic		= 0x403
	Activity	= 50001
	SendWeight	= 250
	LogWeight	= 250
	Context 	= User V2, control at logon session end.

