' INSTALL.SUB for BMULTI 10.1 
'      
'  51789 TEG Update to handle named volume [B25BMU1].
'      
'  41089 TEG change to be applicable to BMULTI Gateway only.
'      
'  32089 TEG change volume names for BMULTI 10.1
'      
'  8988 TEG include <ServiceID> in BMULTI 9.0 command parameters.
'
'  7986 bp  use parameter0 and 1.
'
'  5786 dc  Install file factored per Camarillo. 
'        Seperate files, XEInstall.sub and  Install.Sub
'        call rqInstall.sub with appropriate parameters, then 
'        call this file
'      
'
'      
'
'  5786 dc   Remove 2
'
'
'  32486    Include parameter field for BMULTI Status
'
' 11890     GNC Changes made to reflect R10.1 release
'
LCopy
'File list'   @[B25BMU1]<Unisys>BMultiFiles.list
'[File prefix(es) from]' [B25BMU1]<Unisys> 
'[File prefix(es) to]'  1
'[File suffix(es)]'
'[Overwrite OK?]'  yes
'[Confirm each?]'  
'[Continue on error?]'
'[Verify copy?]'

Copy
[Kbd]
[Sys]<$>args.tmp
y'[Configuration File]'
Copy
[Kbd]
[Sys]<$>desc.tmp
y'Installs the Burroughs Multipoint protocol handler.'
New Command
'Install BMULTI Gateway'
1BmZip.Run
@[Sys]<$>args.tmp
@[Sys]<$>desc.tmp
Yes

0Copy
[Kbd]
[Sys]<$>args.tmp
y'[Configuration File]'
Copy
[Kbd]
[Sys]<$>desc.tmp
y'Creates and maintains BMULTI configuration files.'
New Command
'Configure BMULTI'
1BmFileEdit.Run
@[Sys]<$>args.tmp
@[Sys]<$>desc.tmp
Yes

0Copy
[Kbd]
[Sys]<$>args.tmp
y'[{Node Name}<ServiceID>]'
Copy
[Kbd]
[Sys]<$>desc.tmp
y'Displays status of individual BMULTI stations.'
New Command
'BMULTI Status'
1BmStatus.Run
@[Sys]<$>args.tmp
@[Sys]<$>desc.tmp
Yes

0Copy
[Kbd]
[Sys]<$>args.tmp
y'[<ServiceID>]'
Copy
[Kbd]
[Sys]<$>desc.tmp
y'Deinstalls the Burroughs Multipoint communications handler.'
New Command
'Deinstall BMULTI Gateway'
1BmUnZip.Run
@[Sys]<$>args.tmp
@[Sys]<$>desc.tmp
Yes

0'
Append
[B25BMU1]<sys>FdSys.Version [Kbd]
1Sys.Version
 BMULTI Gateway installed on d|*w *n *d, yyyy, at *t:0m|
'
Video
N


COPY
[kbd]
[VID]
CEF

	
								     
	 AEIMPORTANT UPGRADE INFORMATION                             AA 
								     
	   Upgrading from versions PRIOR to:			     
								     
	   BMULTI 10.2 MAY REQUIRE changes of the RTSCTS, XMTRCV  
		and RTS Hold Delays.  Please refer to the    	     
		Release Notes for details.			     
								     
	   BMULTI 10.1 REQUIRES that the configuration file be      
		updated.  Use the CONFIGURE BMULTI Utility to	     
		OPEN the existing file and the SAVE or FINISH.	     
		This will update the configuration file. 	     
								     
		*** PLEASE READ RELEASE NOTES FOR DETAILS ***	     
	   							     
		     Press AEGOAA to continue the installation.          
								     
	
1
