'
Type
[kbd]PF
Remove the diskette from the floppy drive [f0] and reinsert the
floppy labelled:

    ACNGEN Initialization Diskette 1 of 2AA


Note:

AE    After inserting the diskette, wait until the light on the floppy    
    drive goes off.                                                     
                                                                        
    Then press GO.                                                      AA

1LInstall








'NGEN Initialization Diskette 1 of 2'Copy
[f0]<sys>SysImage.sys
SysImage.sys
yBootstrap
[f0]<sys>sysImage.sys
.
PO	 p@0	0_?
 0PPo'(, 5_50:O:;@=P?0B@COC@DOpE?EF4H|7'