vthlp4ObjIO version X2.4DATAFH
vthlp4	PVT220 Function KeysPage 4PCTOS Key         Description1PF1to F5Sends ESC [ xx  to host$*(xx = 12 for F1, 13 for F2 .... 15 for F5)P	F6 to F101Sends VT220 function key F6 to F10 string to HostFCode_F1 to Code_F10 Sends VT220 function key F11 to F20 string to Host
Shft_F1 to Shft_F107Sends user defined function key string for Function Key F1 to F10 to host, if available.KCode_Shift_F1 to    Sends user defined function key string for Function KeyCode_SHift_F10F11 to F20 to host, if available.PPageSends FIND command to host (ESC [ 1 )SentSends INSERT HERE command to host (ESC [ 2 )Line(Sends REMOVE command to host (ESC [ 3 )Col (Sends SELECT command to host (ESC [ 4 )Para, Prev PageSends PREV SCREEN command to host (ESC [ 5 )Word, Next PageSends NEXT SCREEN command to host (ESC [ 6 )PGoSends FK16 sequence (VT220 DO key)Help$Sends FK15 sequence (VT220 HELP key)PPMNote:    If no user defined function keys are available then the shifted keys	:will not send a sequence to the host. A beep will indicate
	+that no user defined sequence is available.t