:Description:CTOS RAF allows a user to view or control another
workstation or memory partition, over CTOS BNet
II or asynchronous dialup networks.

:StyleId:B25RAFS
:PackageName:RAFSource
:Version:s3.2.2
:RequiredMemory:1000K
:RequiredDiskSpace:1350

:Commands:'RAF Source' 'RAF RS232 Source' 'RAF Source User Profile' 'RAF Script' 'RAF Telephone Directory' 'MP Unload Bridge' 'MP Unload Service' 'MP Load Bridge' 'MP Load Service' 'MP Notification'

:ProductFiles:<Sys>AGPIPM.font <Sys>SG3IPM.font <Sys>B27IPM.font <Sys>IPM.font <Sys>RAFSource.run <Sys>Request.RAF.sys <Sys>RafSourceProfile.sys <Sys>DeInstMPBrdg.run <Sys>DeInstMPSrvr.run <Sys>MPBrdg.run <Sys>MPSrvr.run <Sys>MPTerm.run <Sys>MPBrdg.Msg <Sys>MPRqst.sys <Sys>MPSrvr.Msg <Sys>MPTerm.Msg <Sys>RAFConfig.sys <Sys>RAFProfile.run

:RelatedFiles:  [Sys]<Sys>Request.Sys

:PreInstallJcl:No
:PreInstallReboot:No
:PostInstallJcl:No
:PostInstallReboot:Yesst.RAF.sys <sys>RAFLog.run <sys>RAFQueryChangeTime.run <sys>RafTargetProfile.run <sys>RafTargetProfile.sys <Sys