 Here is a sample Transport.config file for a workstation in a subnet
 128.39.2.0 to 128.39.2.31 of class B network 128.39.0.0

     <== our local ==>       <=== defaults ==>

     name       address      MSS  window   TTL
ident ngen1    128.39.2.5     512   2048     4

             here   slice  interface   mode   MTU
attach ether  master   0      ec0       arpa  1500

 local host entries

             name     address
host add  gateway1    128.39.2.31
host add     ngen2    128.39.2.4
host add       pc1    128.39.2.6

 remote host entries

             name     address
host add     ngen3    128.39.2.33
host add     ngen4    128.39.2.37

 route directly on ethernet to subnet 128.39.2.0  128.39.2.31
 route all other on ethernet to gateway 128.39.2.31
 gateway 128.39.2.31 will route over slip link to gateway 128.39.2.63
 which will route over ethernet on subnet 128.39.2.32  128.39.2.63

            address    bits    gateway   metric interface
route add  128.39.2.32   27   128.39.2.31    0      ec0
route add  128.39.2.0    27     0.0.0.0      0      ec0

