 Here is a configuration file suitable for a workstation that 
 resides in class C network 193.47.35.0

 only one device; an ethernet slice.

     <== our local ==>       <=== defaults ==>
     name       address      MSS  window   TTL
ident sirius    193.47.35.31  512   2048     2

             here   slice  interface   mode   MTU
attach ether  master   0      ec0       arpa  1500

             name     address
host add     ngen1    193.47.35.5
host add     ngen2    193.47.35.4
host add       pc1    193.47.35.6

 only one route; to the only device.

          address     bits  gateway   metric interface
route add  0.0.0.0       0   0.0.0.0     0      ec0

