vthlp1ObjIO version X2.4DATAFHo
vthlp1	PSpecial CTOS KeysPage 1 PCTOS Key         Description1FinishTerminate the Emulatorunless in ANSI modeShift_FinishTerminate the Emulator in all modesCode_Finish	:PCode_Shift_Finish9Clear the Call (Disconnect Line) and enters Config ScreenP	Code_Mark Send a BREAK signal (RS232 only)PCancel)Send ESC character (Vt100 and Vt220 only)Shift_CancelClear Screenand move cursor to HomeCode_Shift_Cancel4Clear Screen, Reset Terminal and move cursor to HomePHelpDisplay Help Info (ANSI and Vt100)
Shift_Help
Display Help Info (All modes)	Code_HelpDisplay Configuration Screen PCode_Shift_QLoad a Function Key file from DiskCode_Shift_TFile Transmit Screen(Code_Shift_F5Function Key definition Screen (Vt100 and Vt220 only)Code_Shift_BClear all User Function Key valuesCode_Shift_SSave current User Function Key valuesCodeK_Shift_R+Restore User Function Keys previously savedPALT orCOMPOSE character key(Dec International only)Code_Shift_Sc_Up:t