***************************************************
***    SAMPLE PARAMETERS FOR  CTOS TCPIP       ***
***  ***
***  CONNECTION LIMITS AND OPERATION MANAGEMENT ***
***************************************************
MaxMaxConn	=	64;
MaxConn 	=	30;
FTPConn		=	5;                * Default for one FTP server.
LHostName	=	HOST1;	          * Site specific.
LHostAddr	=	195.63.74.150;	  * Site specific.
SpecHostAddr	=	0.0.0.0;	  * Site specific.
NetVolume	=	SYS;		      * Site specific.
Log     	=	OFF;
*NetMask	=	255.255.255.128;  * Only needed for sub networks
ReqTrace	=	0;
*LHostAddrX	=	195.63.72.151;	  * Site specific  Dual IP X.25 
			                      * address
BroadcastAddr	=	0.0.0.255;	  * Site specific  UDP broadcast 
			                      * address

************************************
***  REMOTE HOST IDENTIFICATION  ***
************************************

RemHostName	=	LOCAL;	        * a LOCAL MUST be specified  the 
			                    * RemHostAddr
RemHostAddr	=	195.63.74.150;	* MUST be the same as in the 
			                    * LHostAddr.
NetType	=	1;                  * NetType 1 = Ethernet LAN

*RemHostName=	XLOCAL;	        * an XLOCAL MUST be specified if X.25 
			                    * is being used  the RemHostAddr
*RemHostAddr=	195.63.72.151;	* MUST be the same as in the 
			                    * LHostAddrX. 
*NetType	=	2;	            * NetType 2 = X.25

RemHostName	=	HOST2;
RemHostAddr	=	195.63.72.152;
NetType	=	2;

RemHostName	=	HOST3;
RemHostAddr	=	195.63.72.153;
NetType	=	2;

RemHostName	=	HOST4;
RemHostAddr	=	195.63.72.154;
NetType	=	2;

RemHostName	=	HOST5;
RemHostAddr	=	195.63.74.151;
NetType	=	1;

RemHostName	=	HOST6;
RemHostAddr	=	195.63.74.152;
NetType	=	1;

RemHostName	=	HOST7;
RemHostAddr	=	195.63.74.153;
NetType	=	1;

***************   END OF FILE  **************PP6S66PP6PP6S66PP6Tt+J;tTt+J;uF6Fu3PPF