vthlp5ObjIO version X2.4DATAFHa
vthlp5	aPRaVT100200 Keypad KeysPage 5PPCTOS Key         Description1Keypad Program Function Key PF1 (ESC [ P)Keypad xProgram Function Key PF2	(ESC [ Q)Keypad Program Function Key PF3	(ESC [ R)Keypad Program Function Key PF4	(ESC [ S)PKeyPad 0KeyPad 0 (ESC [ p)*KeyPad 1KeyPad 1 (ESC [ q)*KeyPad 2KeyPad 2 (ESC [ r)*KeyPad 3KeyPad 3 (ESC [ s)Note:See Help Page 9 for detailsKeyPad 4KeyPad 4 (ESC [ t)on Keypad usage on theKeyPad 5KeyPad 5 (ESC [ u)K1 style keyboard.
KeyPad 6KeyPad 6 (ESC [ v)*KeyPad 7KeyPad 7 (ESC [ w)*KeyPad 8KeyPad 8 (ESC [ x)*KeyPad 9KeyPad 9 (ESC [ y)*PKeyPad +KeyPad Minus
 (ESC [ m)Note: These keys are chosen KeyPad =KeyPad Comma
 (ESC [ l)
to ensure same physicalKeyPad .KeyPad Period
 (ESC [ n)	layout as VT100.Keypad ENTERKeyPaKed Enter	(ESC [ M)PJNote that the standard keypad characters are enabled only if the keypad isKturned on. If the keypad is turned off, the above sequences can be sent by 6pressing the CODE key with the appropriate keypad key.The keypad is turned onKor off with either the Config Screen or via Escape sequences from the host.t