;
;	Plog Message File
;
;	This file contains the error and text messages used by the Plog
;	Utility. This file may be edited to change the text of any
;	messages issued by Plog. The utility Create Message File
;	is provided to build a binary formatted binary text file which is 
;	read by Plog. 
;
;	The syntax of this is described below. Each message in the file
;	is defined by
;
;	<colon>nnnnn<colon>  <delim> Text <delim>
;
;	
;	
;	Macro expansion syntax
;
;	Macro	String to be inserted
;
;	U		workstation user name.
;	Dn		system datetime formatted with template number n.
;	Kn		keycap text for key number n.
;	nD		nth parameter as datetime
;	nN		nth parameter as unsigned integer
;	nS		nth parameter as a string
;	n		nth parameter as a string
;

;
;	Keycap Text definitions 
;
;	Name		Number		Text
;	============================
;	Action		1			ACTION
;	Backspace	2			BACK SPACE
;	Bound		3			BOUND
;	Cancl		4			CANCEL
;	Code		5			CODE
;	Copy		6			COPY
;	Delete		7			DELETE
;	Finish		8			FINISH
;	Go			9			GO
;	Help		10			HELP
;	Lock		11			LOCK
;	Mark		12			MARK
;	Move		13			MOVE
;	Next		14			NEXT
;	NextPage	15			NEXT PAGE
;	OverType	16			OVER TYPE
;	PrevPage	17			PREV PAGE
;	Return		18			RETURN
;	ScrlDown	19			SCROLL DOWN
;	ScrlUp		20			SCROLL UP
;	Shift		21			SHIFT
;	Tab			22			TAB
;
;
:35051: PLog 
:35052: BUFFER OVERFLOW  
:35053: CONFIGURATION ERROR  
:35054: COMMIOP ERROR  
:35055: MINI CLUSTER ERROR  
:35056: SRP CLUSTER ERROR  
:35057: DISK ERROR  
:35058: TAPE ERROR  
:35059: SUCCESSFUL TAPE SERVER INSTALLATION       
:35060: SYSTEM INITIALIZATION ERROR  
:35061: SYSTEM BOOT  
:35062: SYSTEM CRASH  
:35063: MESSAGE TEXT LOGGED  
:35064: SRP Print Log  Version 
:35065: ,  Line: 
:35066: Line: 
:35067: , Id: 
:35068:  Unit 
:35069: ERC = 
:35070: Also: 
:35071: Number of Retries: 
:35072: Recovered
:35073: Unable to Recover
:35074: Volume Name: 
:35075: Number of occurrences since last similar Log entry: 
:35076: Command: 
:35077: Initialization Status: 
:35078: Error detected in: 
:35079: Primary Status: 
:35080: Main Status: 
:35081: Error Status: 
:35082: Secondary Status: 
:35083: Os Booted: 
:35084: Crash Information: 
:35085: Winchester
:35086: Floppy
:35087: SCSI drive
:35088: SMD drive
:35089: IWS,  
:35090: AWS210,  
:35091: AWS230,  
:35092: AWS240,  
:35093: NGENT1,  
:35094: NGENT2,  
:35095: 286i,  
:35096: CWS,  
:35097: Unknown Hardware,  
:35098: Standalone
:35099: Cluster
:35100: Master
:35101: Unknown Cluster Type
:35102:  WorkStation
:35103: ,  With 
:35104: ,  No 
:35105: Iop
:35106: CommIop
:35107: File System
:35108: Memory Size: 
:35109: SignOn User Name: 
:35110: Volume: 
:35111: Cylinder: 
:35112: ,  Head: 
:35113: ,  Sector: 
:35114: , Alignment: 
:35115: ,  Number of Sectors: 
:35116: CommIop Number: 
:35117: Log File information does not agree with Home Block
:35118: Volume has zero length log file, nothing logged
:35119: No video hardware
:35120: DMA failure when loading font
:35121: DMA failure when reading font
:35122: Font checksum error
:35123: Memory test failed
:35124: Bus timeout test failed
:35125: Parity test failed
:35126: No keyboard hardware
:35127: Keyboard reset error
:35128: Keyboard ROM checksum error
:35129: Keyboard loopback test failed
:35130: Keyboard interrupt test failed
:35131: Real Time Clock test failed
:35132: Programmable Interrupt Timer test failed
:35133: Continuous Programmable Interrupt Timer interrupts
:35134: Communications hardware test failed
:35135: Cluster workstation timed out
:35136: Invalid state, run the crash dump analyzer
:35137: Communications hardware failure, run comm diagnostic
:35138: Protocol failure detected by master workstation
:35139: Bad DMA Buffer address
:35140: Invalid card bit
:35141: Busy bit IO
:35142: Protocol failure detected by cluster workstation
:35143: Hardware error
:35144: Master workstation disconnect
:35145: Request block error
:35146: Bootstrap failure
:35147: No available IDs
:35148: ID search failure
:35149: Disconnect during WS boot: not enough X Buffers
:35150: Operation aborted
:35151: Cluster DMA transfer: input buffer length exceeded
:35152: CommIop time out, run CommIop diagnostic
:35153: Line not configured, check system build parameters
:35154: CommIop not loaded. Missing [sys]<sys>CommIop>sysImage.sys
:35155: CommIop loading error, run CommIop diagnostic
:35156: Invalid CommIop data structure, take crash dump and run CommIop diagnostic
:35157: CommIop restart due to carrier problems
:35158: CommIop channel hold due to carrier problems
:35159: CommIop command failure, bad control info passed from CommIop to master ws
:35160: Bad command passed from master workstation to CommIop
:35161: CommIop bootstrap checksum failure
:35162: The Multibus interface hardware on the CommIop is not functional
:35163: The CommIop received an unknown interrupt
:35164: CommIop RAM failure in writeread test
:35165: CommIop RAM failure  invalid bit set
:35166: CommIop RAM failure  invalid bit cleared
:35167: CommIop RAM failure in addressing test
:35168: CommIop handler time out, no info from master
:35169: Invalid check word in CommIop queues, run memory test on master
:35170: CommIop RAM checksum error, run CommIop diagnostic
:35171: Invalid entry in CommIop queue
:35172: Invalid CommIop buffer pointer
:35173: CommIop carrier problem
:35174: CommIop software inconsistency
:35175: CommIop timer failure
:35176: CommIop DMA failure
:35177: CommIop SIO static test failure
:35178: CommIop SIO functional test failure
:35179: Cluster too heavily loaded
:35180: Workstation timed out, did not respond
:35181: Workstation down, CRC errors detected
:35182: Workstation down, overrun errors detected
:35183: Workstation down, invalid SDLC frames received
:35184: Invalid SDLC protocol
:35185: CWS time out, no response
:35186: CWS CRC errors, run Comm and CommIop diagnostics
:35187: CWS overrun error, check system build parameters
:35188: Bad SDLC protocol
:35189: Cluster workstation requested disconnect
:35190: ISAM DATA STORE ERROR  
:35191: ISAM INDEX ERROR  
:35192: ISAM INDEX TO DATA STORE ERROR  
:35193: Data set: 
:35194: Uri: 
:35195: Crash
:35196: Boot
:35197: Init
:35198: ISAM
:35199: Disk
:35200: Config
:35201: Tape
:35202: Mini
:35203: Invalid type parameter
:35204: Description: 
:35205: Memory protection fault detected
:35206: Bus timeout detected
:35207: Double bit memory error detected
:35208: Memory parity fault detected
:35209: The memory location being referenced was 
:35210: The contents of the above memory location were 
:35211: Power failure detected
:35212: Unknown nonmaskable interrupt encountered
:35213: Stray interrupt of type 0N detected
:35214: Divide overflow detected
:35215: Remote double bit error or reference to remote nonexistent memory detected 
:35216: Executing instruction preceeding location 
:35217: Invalid data command, head out of bounds 
:35218: Invalid data command, sector out of bounds 
:35219: Invalid data command, cylinder out of bounds 
:35220: Invalid data command 
:35221: Drive became not ready during data 
:35222: Drive not ready for data 
:35223: Drive Fault detected 
:35224: Drive not ready when issuing Command 
:35225: Equipment check during data 
:35226: Data late 
:35227: CRC error in data field 
:35228: CRC error in ID field 
:35229: Halt during command execution 
:35230: Read error 
:35231: Abnormal termination of IO 
:35232: Tried to access a sector beyond the end of a cylinder 
:35233: No Data, wrong cylinder 
:35234: No Data, bad cylinder 
:35235: Sector not found 
:35236: Cylinder compare error 
:35237: Head compare error 
:35238: No Data
:35239: OverRun error
:35240: The disk is write protected
:35241: Tape is write protected
:35242: Drive was Busy when issuing command 
:35243: Missing address mark in data field 
:35244: Missing ID field address mark 
:35245: Controller readwrite error 
:35246: IO Error, 
:35247: Error Type 
:35248: Command in execution 
:35249: Seek never completed 
:35250: Controller waiting for data 
:35251: Data address mark not found 
:35252: Track 0 not found after recal 
:35253: Command aborted by controller 
:35254: Bad block mark was detected 
:35255: Controller busy after interrupt 
:35256: Data lost in transfer tofrom controller 
:35257: Sector not found 
:35258: Deleted record flag set 
:35259: Seek error 
:35260: HalfInch Tape
:35261: Qtr Inch Cartridge
:35262: Tape Server failed to installSee error code above
:35263: Number of Tape Buffers allocated: 
:35264: Size in bytes of each Tape Buffer: 
:35265: Number of soft errors in current ReadWrite operation: 
:35266: Status bytes: 
:35267: Hardware status: 
:35268: Current Error conditions  Status: 
:35269: File Mark encountered 
:35270: Hard tape error 
:35271: Corrected tape error 
:35272: End of Tape
:35273: Beginning of Tape
:35274: Tape drive not online 
:35275: High speed selected
:35276: Low speed selected
:35277: Data Busy asserted 
:35278: Tape is currently rewinding 
:35279: Tape not ready 
:35280: Formatter is busy 
:35281: Cumulative IO errors in current Session: 
:35282: Cumulative corrected IO errors in current Session: 
:35283: Block In Error not located 
:35284: Unrecoverable data error 
:35285: Cartridge not inserted 
:35286: ResetPowerUp occurred 
:35287: Eight or more Read retries 
:35288: No Data Detected 
:35289: Illegal command 
:35290: Cumulative Underruns in current Session: 
:35291: Cumulative Marginal reads in current session: 
:35292: Tape operation timed out.
:35293: Tape IO Error.
:35294: Tape Hardware Error.
:35295: SRP Winchester
:35296: SRP Cartridge
:35297: SRP SMD drive
:35298: Main Status: 
:35299: Error Status: 
:35300: Misc Status: 
:35301: odd
:35302: even
:35303: File Processor
:35304: Terminal Processor
:35305: Cluster Processor
:35306: Storage Processor
:35307: TIA Processor
:35308: Storage Processor with Storage Controller (DP)
:35309: Applications Processor
:35310: Unknown Processor Type
:35311:  in slot 
:35312:  on line 
:35313: Configuration file error in file 
:35314: (No Include Name)
:35315: (Unterminated String)
:35316: (Unable to open include file)
:35317: (Null Field)
:35318: (Keyword requires argument)
:35319: (Misplaced quote)
:35320: (Include nesting limit exceeded)
:35321: Error initializing 
35322 Not Used
:35323: Sector field not found (bad Cmd or bad track)
:35324: Data address mark error, probably CRC
:35325: Track 0 error during recal operation
:35326: Attempted to access sector marked as bad
:35327: Fault detected during disk DMA transfer
:35328: Write fault error 
:35329: Invalid year given in datetime parameter
:35330: Invalid day given in datetime parameter
:35331: Date and day of week disagree in datetime parameter
:35332: Invalid time given in datetime parameter
:35333: No Sense, 
:35334: Recovered from error, 
:35335: Unit not ready, 
:35336: Medium error, 
:35337: Hardware error, 
:35338: Illegal Request, 
:35339: Unit Attention, 
:35340: Data protect, 
:35341: Blank check, 
:35342: Vendor Unique, 
:35343: Copy aborted, 
:35344: Aborted Command, 
:35345: Equal, 
:35346: Volume overflow, 
:35347: MisCompare, 
:35348: Reserved, 
:35349: Seek error 
:35350: Recovered with retries 
:35351: Recovered with ECC 
:35352: Recovered DAM error 
:35353: Recovered ID AM error 
:35354: Defect list is full 
:35355: Drive not ready 
:35356: Drive doing recal 
:35357: Drive spinning up 
:35358: Waiting for START command 
:35359: Data CRC or ECC error 
:35360: Uncorrectable data error 
:35361: No Synch field 
:35362: Illegal Synch field 
:35363: No index signal 
:35364: Drive write fault 
:35365: Address mark not found 
:35366: Bad defect list format 
:35367: Target was reset 
:35368: Drive internal timeout 
:35369: Drive firmware error 
:35370: Invalid command 
:35371: Illegal block address 
:35372: Illegal argument 
:35373: Invalid Logical Unit number 
:35374: Bad parameter list 
:35375: Usage counter overflow 
:35376: Starting block address: 
:35377: Error block address: 
:35378: Sense Bytes: 
:35379: , returned erc = 
:35380: NGENT3,  
:35381: ????
:35382: Message
:35383: 386i,  


Reserve message numbers through 35400 for Plogon 
:35230: Read error 
:35231: Abnormal termination of IO 
:35232: Tried to access a sector beyond the end of a cylinder 
:35233: No Data, wrong cylinder 
:35234: No Data, bad cylinder 
:35235: Sector not found 
:35236: Cylinder compare error 
:35237: Head compare error 
:35238: No Data
:35239: OverRun error
:35240: The disk is write protected
:35241: Tape is write protected
:35242: Drive was Busy when issui