
VTPKEYS1ObjIO version X2.4DATAFHaVTPKEYS1	P
;
8  BTOS  VT Emulator  Programmable Key Definition      
;
PPPKey 1:2:3:4:5:6:7:8:9:0:PLYou may enter special characters (such as Carriage Return or Line Feeds) as Ocontrol characters in for format ^x (where x is in the range az). For example,A^J will send a Line Feed Character (equal to Control J  Hex 10).PP0Enter the data and press GO or CANCEL to dismiss @E@E@E	@E
@E@E@E
@E	@E
@EVT_Key
t