' Install.Sub <B25CE11>  MOD 121787, R. Askren 
2Copy
[Kbd]
[Vid]
PF

		    
		    	BTOS C Compiler Installation	
		    

	  If this is the master station of a cluster system, then power
	  down all cluster workstations.

	  If this is a cluster workstation, then power down all other
	  workstations except this station and the master station.


			    PRESS AE<GO>AA when ready
			    1				
Copy
[Kbd]
[Vid]
PF

	
									
	    BTOS C Compiler files will be installed on your [Sys]	
		 volume in directories <Sys> and <BTOSC>.		
									
				PRESS AE<GO>AA to continue.			
									
	
1Copy
[Kbd]
[Vid]
PF

	
									
	    Volume Status will display the number of unused sectors	
		 on your [Sys] volume.					
									
	    AFPRESS AE<GO>AA to invoke Volume Status, note the number of	
		 unused sectors, then AFPRESS AE<GO>AA again to continue.	
									
	
1Screen Setup

yesVolume Status
Sys1Copy
[Kbd]
[Vid]
PF

	
									
	    C Compiler requires approximately 2200 sectors on a	
		 BTOS workstation.					
									
	    If this system does not have the required space available	
		 AFPRESS AE<ACTION><FINISH>AA to cancel installation.		
									
	    If this system does have the required space available	
		 AFPRESS AE<GO>AA to continue.				
									
	
1?2Copy
[Kbd]
[Vid]
PF

		    
		    	BTOS C Compiler Installation	
		    

	    Power down all other workstations except this station and
	    the XE520 master.

			    PRESS AE<GO>AA when ready
			    1				
Copy
[Kbd]
[Vid]
PF

	
									
	    BTOS C Compiler files will be installed on your [Sys]	
		 volume in directories <Sys> and <BTOSC>.		
									
				PRESS AE<GO>AA to continue.			
									
	
1Copy
[Kbd]
[Vid]
PF

	
									
	    Volume Status will display the number of unused sectors	
		 on your [Sys] volume.					
									
	    AFPRESS AE<GO>AA to invoke Volume Status, note the number of	
		 unused sectors, then AFPRESS AE<GO>AA again to continue.	
									
	
1Screen Setup

yesVolume Status
Sys1Copy
[Kbd]
[Vid]
PF

	
									
	    C Compiler requires approximately 2200 sectors on the	
		 XE520 master.						
									
	    If the system does not have the required space available	
		 AFPRESS AE<ACTION><FINISH>AA to cancel installation.		
									
	    If the system does have the required space available	
		 AFPRESS AE<GO>AA to continue.				
									
	
1Create Directory
2[Sys]?2[Sys]<BTOSC>LCopy
CC1.Run CC2.Run CC3.Run CC4.Run
[B25CE11]<Unisys>
2[Sys]?2[Sys]<Sys>

yesCopy
[kbd]
[vid]
PF




	
									
		  Remove the disk from the floppy disk drive and	
		  insert C Compiler software disk number 2 of 3.	
									
	

			      PRESS AE<GO>AA when ready
			1					
LCopy
CC0.Run
[B25CE12]<Unisys>
2[Sys]?2[Sys]<Sys>

yesLCopy
[B25CE12]<Unisys>*.Lib

2[Sys]?2[Sys]<BTOSC>

yesLCopy
[B25CE12]<Unisys>*.Lnt

2[Sys]?2[Sys]<BTOSC>

yesLCopy
[B25CE12]<Unisys>*.Obj

2[Sys]?2[Sys]<BTOSC>

yesLCopy
[B25CE12]<Unisys>*.h

2[Sys]?2[Sys]<BTOSC>

yesCopy
[kbd]
[vid]
PF




	
									
		  Remove the disk from the floppy disk drive and	
		  insert C Compiler software disk number 3 of 3.	
									
	

			      PRESS AE<GO>AA when ready
			1					
LCopy
[B25CE13]<Unisys>*.Lib

2[Sys]?2[Sys]<BTOSC>

yesNew Command
'CCompiler'
2[Sys]?2[Sys]<Sys>CC0.Run
'[Options]' 'Filename'
'Invoke the C Compiler for the file specified.'
yes

0Append
[B25CE13]<Sys>fdSys.Version [Kbd]
2[Sys]?2[Sys]<Sys>Sys.Version C Compiler installed on d|*w *n *d, yyyy, at *t:0m|
2Copy
[kbd]
[vid]PF


	   AE ***** INSTALLATION OF BTOS C COMPILER COMPLETE ***** AA


	Please remove the C Compiler diskette from the floppy disk drive
	and put it and all other software diskettes in a safe place.

	If this is a cluster system, you may now resume cluster operations.
PN

	  If this is the master station of a cluster system, then power
	  down all cluster workstations.

	  If this is a cluster workstation, then power down all other
	  workstations except this station and the master station.


			    PRESS AE<GO>AA when ready
			    1				
Copy
[Kbd]
[Vid]
