
         
UNISYS
	Emergency 	Maintenance 	Update
	
	CTOS BMULTI s10.4.50
October 23, 1997
	Released Version:	10.4.0
	Style ID:	B25BMU

	DESCRIPTION

This Emergency Maintenance Update (EMU) is provided on an asneeded basis only.  It is not an official release nor is it available through Corporate Software and Publications Operations (CSPO).  The information in this document is supplemental to the product's Software Release Announcement (SRA).
Contact your Unisys support center for more information concerning this EMU.

RESTRICTIONS
There are no new restrictions added with this EMU.

SOFTWARE FILES
This EMU is a complete replacement package for the released product.

INSTALLATION INSTRUCTIONS
Use Installation Manager or Software Install to install the EMU on each system requiring the updated software.

PROBLEMS CORRECTED

EMU s10.4.50 is created to remove problem with Bmulti Line Monitor on VAM 4.4 

EMU s10.4.09 is created to remove some problems introduced when creating the earlier EMU, s10.4.08. With BMULTI s10.4.08, the Status Monitor and BMulti Agent Configurator exit with error 3700. BMULTI s10.4.08 used a later version of Forms library and forms built using earlier version of Forms Designer software were not readable. 

BMULTI LINE MONITOR
PLEs fixed in s10.4.50

PLE  17084879	BMULTI Monitor will not work with VAM 4.4 OK with 4.3 and 
                Bmulti Line monitor does not display characters

BMULTI GATEWAY  
PLEs fixed in s10.4.08
PLE 16513351	BMULTI crashes with erc 80 in EnableSIOXmt.
PLEs fixed in s10.4.07
PLE 16459470	Page fault during interrupt processing (BMULTI) results in crash 13960.
PLEs fixed in s10.4.05
PLE 16182222	BMULTI NAKs host selects after a fast select is sent to a device on another drop of a split line.

HIGHLEVEL PROCEDURAL INTERFACE (HLI) LOWLEVEL PROCEDURAL INTERFACE (LLI)
PLEs fixed in s10.4.05
PLE 16159751	(HLI) The write status did not get updated from write initiated (01) to write compete (16).

BMULTIX25
PLEs fixed in s1.4.07
PLE 16585408	Can Not Open VC with BMX25 after the Modem Line Goes Down (On a multiprocessor system).
PLE 16574104	IOP crash with 65300 when no corresponding X25 remote address.
PLEs fixed in s1.4.06
PLE 16451061	Problems are encountered when using large messages with BMX25.

BMUTLISuspendResume

PLEs fixed in s1.3.05
No Changes
BMULTI AGENT

PLEs fixed in s10.4.08
No Changes

BMULTI LINE MONITOR
PLEs fixed in s10.4.50

PLE  17084879	BMULTI Monitor will not work with VAM 4.4 OK with 4.3 and 
                Bmulti Line monitor does not display characters

