@
@These are the messages added for status codes reporting.  
@They have been officially allocated with SanJose for Message Posting product.
@These are only used to indicate the error conditions.   
@Status codes 40219 to 40223 are for Message Posting Notification.
@Status code 40224 is used to indicate failure to load the message file
@and is common for all three components of Message Posting. Do not use it here.
@
40219Error :Fatal Error 
@*
@These are the help messages for Message Posting Terminal program.
@Message nos. are followed by the message text.
@No help message con be grater than 1024 characters including CRLFs.
@A single line in a message should not exceed 70 characters including CRLF.
@*
@
14ERROR : No Message is Available for message no. 0
33ERROR : Service Not Available.
@*
@The messages for Distribution list help form follow.
@The message nos. reserved are : 42000 to 42004
@*
42000   Dist_List Help@ Specify max. 21 characters.
42001@.......
The distribution list contains a list of node name  user name pairs. 
Current message can be sent to all these pairs.

Enter name of distribution list and press :

 GO       to Send the message.
 CANCEL   to Return to previous state.
 FINISH   to Terminate.
@
42002PRESS ANY KEY TO CONTINUE..........
@
@*
@The messages for EMHelp form follow.
@The message nos. reserved are : 42005 to 42009
@*
42005  WORKSTATION HELP@ Specify max. 21 characters.
42006@.......
The Terminal screen allows you to enter a message and Send it
OR Retrieve a previously stored message and send it
OR Enter and Store a message for future use.

LOCAL : Press  F1  to send message to local users.
NET   : Press  F2  to send message to remote node and user.
ALL   : Press  F3  to send message to all nodes and users.
@
DLIST : Press  F4  to send message using distribution list.
SAVE  : Press  F9  to store message for later recall.
RECALL: Press  F10  to recall previously stored message.
@

Press  CANCEL  to clear the message form.
Press  FINISH  to exit the program.
Press  GO      to send the message.
@
42007PRESS ANY KEY TO CONTINUE..........
@
@*
@The messages for GNXHelp form follow.
@The message nos. reserved are : 42010 to 42014
@*
42010   NODE NAME HELP@ Specify max. 21 characters.
42011@.......
Enter the name of remote node to whom you wish to send the message.


UPDATE         : Press  UPDATE  to reflect the current information.
GO             : Press  GO  to send message to remote node and user.
@
42012PRESS ANY KEY TO CONTINUE..........
@
@*
@The messages for GNYHelp form follow.
@The message nos. reserved are : 42015 to 42019
@*
42015   NODE NAME HELP@ Specify max. 21 characters.
42016@.......
Select remote node to whom you wish to send a message and press  GO 


, , ,       : Press these keys to traverse around  the screen,
                  highlighting  the currently selected remote node.

Press  GO  to send the message to the selected remote node.

Press  CANCEL  OR  FINISH  to dismiss this function.
@
42017PRESS ANY KEY TO CONTINUE..........
@
@*
@The messages for GUXHelp form follow.
@The message nos. reserved are : 42020 to 42024
@*
42020   USER NAME HELP@ Specify max. 21 characters.
42021@.......
Select the name of user to whom you wish to send a message.


, , , ,  Scroll UP  :Press combination of these keys to select
    and      Scroll DN  :name of a user

ALL                     :Press  F1  to send message to all users.
UPDATE                  :Press  F10  to reflect current information.
@
42022PRESS ANY KEY TO CONTINUE..........
@
@*
@The messages for Help Template form follow.
@The message nos. reserved are : 42045 to 42049
@*
42045HELP@ Specify max. 21 characters.
42046Press any key to exit.
@
@*
@The messages for INet Help form follow.
@The message nos. reserved are : 42025 to 42029
@*
42025NETWORK HELP@ Specify max. 21 characters.
@Press <F1> to access remote node through Micro Accord. modified 42026 milind
42026@.......

Press  F2  to access remote node through BNet.

Press  CANCEL  OR  FINISH  to dismiss this function.
@
42027PRESS ANY KEY TO CONTINUE..........
@
@*
@The messages for ISM Help form follow.
@The message nos. reserved are : 42030 to 42034
@*
42030 STORE MESSAGE HELP@ Specify max. 21 characters.
42031@.......
You can assign one of the function keys from  F1  to  F10  to hold a 
stored message. 
Enter a name for a message in the function key label area.  
Overtype, if you are replacing a previously stored message.

Press function keys  F1  to  F10  that you wish to have  
the message correspond to.
@
42032PRESS ANY KEY TO CONTINUE..........
@
@*
@The messages for NoHelp form follow.
@The message nos. reserved are : 42035 to 42039
@*
42035NO HELP@ Specify max. 21 characters.
42036THERE IS NO HELP AVAILABLE AT THIS POINT.
42037PRESS ANY KEY TO CONTINUE...........
@
@*
@The messages for RMHelp form follow.
@The message nos. reserved are : 42040 to 42044
@*
42040   RECALL MSG HELP@ Specify max. 21 characters.
42041@.......
Recall a previously stored message.

Press a function key from  F1  to  F10 , to recall the corresponding 
previously stored message.
42042PRESS ANY KEY TO CONTINUE...........
@
@*
@The messages for SMHelp form follow.
@The message nos. reserved are : 42045 to 42049
@*
42045   STORE MSG HELP@ Specify max. 21 characters.
42046@.......
Assign a message to each of the function keys from F1 to F10.
Press desired function key that this message shall be assigned to and 
Enter a name for the message in the function key label area.

Press function key F1 to F10 that you wish to have the message stored under.
Press  CANCEL  OR  FINISH  to dismiss this function.
Press  GO  to confirm.
@
42047PRESS ANY KEY TO CONTINUE...........
@
@*
@The messages for GNCHelp form follow.
@The message nos. reserved are : 42050 to 42054
@*
42050   NODE NAME HELP@ Specify max. 21 characters.
42051@.......

Enter the name of remote node to whom you wish to send the message.

Press  GO  to send message to remote node and user.
@
42052PRESS ANY KEY TO CONTINUE..........
@
@*
@The messages for Error form follow.
@The message nos. reserved are : 42060 to 42064
@*
42060ERROR @Specify max. 20 chars.
42061Error Code    :@ Specify max. 16 characters.
42062Error Msg     :@ Specify max. 16 characters.
42063PRESS ANY KEY TO CONTINUE..........@ Specify max. 60 characters.
@
@*
@The messages for Message form follow.
@The message nos. reserved are : 42065 to 42084
@*
42065
42066Message No :@ Specify max. 12 characters.
42067From       :@ Specify max. 12 characters.
42068DateTime  :@ Specify max. 12 characters.
42069Acknowledgement         [YN]:@ Max. 31 characters
42070Acknowledgement Warning [YN]:@ Max. 31 characters
42071Distribution List Name       :@ Max. 31 characters
@
42075WORKSTATION@ Max. 11 characters
42076  MESSAGE  @ Max. 11 characters
42077   TEXT    @ Max. 11 characters
@*
@The messages for Nodes form follow.
@The message nos. reserved are : 42085 to 42089
@*
42085NodeNames@ Max. 21 characters
42086Update@ Max. 6 characters
@
@*
@The messages for One Node form follow.
@The message nos. reserved are : 42095 to 42099
@*
42095   Node Selection@ Max. 21 characters
42096Node Name@ Max. 12 characters
@
@*
@The messages for Overlay form follow.
@The message nos. reserved are : 42100 to 42104
@*
42100
@
@*
@The messages for Users form follow.
@The message nos. reserved are : 42120 to 42124
@*
42120      User Name@ Max. 21 characters
@
@*
@The messages for function key labels follow.
@The message nos. reserved are : 42130 to 42149
@Specify max. 6 characters for the function key labels.
@*
42130Local
42131Net
42132All
42133DList
42134Save
42135ReCall
42136Users
42137Msg
42138mAcord
42139BNet
42140Update
42141@CTNet
42142      
@
@*
@The messages for general terminal functions follow.
@The message nos. reserved for errors are : 42150 to 42199
@The error message follow now.
@Specify max. 70 characters per line including CRLF and parameters strings.
@*
42150Error : Cannot save the message.
42151Error : No message stored.
42152Error : No users for this node.
42153Error : No remote nodes.
42154Error : You must enter a node name.
42155Error : MicroAccord is not installed.
@
42156Error : Unable to send message to everyone.
42157Error : Unable to send message to node  user {0}1
42158Error : Unable to send message to users on the node {0}
42159Error : Unable to send message to node  user {0}1
@
42160Error : Message file in use.
42161Error : Unable to create message file.
42162Error : Unable to open message file.
@ 
@@@ Added this message if BNet error in accessing node, Ravi Govil
42163Error : Unable to access the specified Node.
@
42165Error : Unable to open Distribution List.
42166Error : Unable to send acknowledgement to node  user {0}1
@
@*
@The message nos. reserved for General Message Posting Messages : 42200 to 
@42249
@These messages follow now.
@*
42200Version 0 1 @Specify the Version no. and date as parameters.
42201Message Posting Bridge  0 loaded.@Specify the Version no. as param.
42203Message Posting Service 0 loaded.@Specify the Version no. as param.
@
@*
@The message nos. reserved for Help  Prompts : 42210 to 42249
@The helpprompt messages follow now.
@Specify max. 70 characters per line including CRLF and parameters strings.
@*
42210 Recall message.
42211 Press a function key to select network.
42212 Select a node name and press  GO  to send message,  CANCEL  to deny.
42213 Select user name and press  GO  to send message,  CANCEL  to deny.
42214 Press a function key for the message.
@
42215 Enter message name and press  GO .
42216 Enter message and press a function key,  FINISH  to exit....
42217 Enter a node name and press  GO .
42218 Sending the message to every one.
42219 Sending the message to the node  user {0}1
@
42220 Sending to all users on the selected node {0}
42221 The message has been sent to everyone.
42222 The message has been sent to the node  user {0}1
42223 The message has been sent to all users on the node {0}
42224
@
42225NoName@ Max. 8 characters
42226Master@ Do not change this.
@
42227 Enter name of Distribution List and Press  RETURN .....
42228 Press :  GO  to send message,  CANCEL  to deny. 
42229 The acknowledgement has been sent to the node  user {0}1
42230
42231 Press  GO  to send the message to all the users,  CANCEL  to deny
42453Error :Message Posting Service was not loaded.
