'*****************************  H E A D E R  ********************************
'**                                                                        **
'** TITLE:        Installation of BMULTI                                   **
'**                                                                        **
'** FILE ID:      [B25BMU1]<Sys>XEInstall.Sub                             **
'**                                                                        **
'** FUNCTION:     This submit file will ...                                **
'**                                                                        **
'** INPUT:        0    The name of the command file to update  NOT      **
'**                      used.                                             **
'**                                                                        **
'**               1    The [volume]<directory> where the files are to    **
'**                      loaded.                                           **
'**                                                                        **
'** OUTPUT:	   0  The [Vol]<Dir>FileName of the loadable request file **
'**                                                                        **
'** CALLED BY:    XESoftware Installation                                  **
'**                                                                        **
'** CALLSUSES:   [B25BMU1]<Sys>rqInstall.Sub                             **
'**		   	   [B25BMU1]<Sys>BmInstall.Sub				   				**
'**		   	   [B25BMU1]<Sys>BmxInstall.Sub			    			**
'**		   	   [B25BMU2]<Sys>InstallBmultiAgent.Sub		    		**
'**		   	   [B25BMU2]<Sys>InstallBmultiAgent.Sub		    		**
'**                                                                        **
'** HISTORY:                                                               **
'**                                                                        **
'** mmddyy  Who     Description                                          **
'**                                                  **
'** 041289  T.Graber Update to be same as Install.sub		    		**
'** 072189  T.Graber Now prompt and wait for user to change the 	    	**
'**                    [Sys]<Sys>Request.Sys entry.			    		**
'** 110790  GNC Added Optional Installation of SuspendResume Filter    	**
'** 042492  Vish     Changed to handle installation via 3 disks          **
'**                                                                        **
'****************************************************************************
'
copy
[kbd]
[vid]

CEF





     AEPLEASE POWER DOWN ALL CLUSTERS THAT BOOTED FROM THIS XE SYSTEMAA


			    AE Press <GO> When Ready AA1
'  'Copy
'      File from       '[Kbd]
'      File to         '[Vid]
'      [Overwrite ok?] '
'      [Confirm each?] '
'   GO''
'
'[Kbd] = '
PF

									      
              AE UNISYS  PRODUCT  INSTALLATION FOR BMULTI R10.4 AA		      
                                                                    	      
                                                                    	      
              THIS SYSTEM MUST BE RUNNING XE CTOS MU2 OR HIGHER.    	      
									      
									      
	  If you are running an older OS then press  AE ActionFinish AA.	      
	  Otherwise: press AE GO AA to continue software installation.	      
                                                                    	      
1
'
Video
N
COPY
[kbd]
[VID]
CEF

	AE							      AA
	AE AA							     AE AA
	AE AA  The installation process will next display the Release    AE AA
	AE AA          Notes. This file contains configuration           AE AA
	AE AA  addenda, as well as information on new features.          AE AA
	AE AA							     AE AA
	AE AA  It is strongly recommended that you read this file at     AE AA
	AE AA  some time prior to executing the Configure BMULTI or the  AE AA
	AE AA  Install BMULTI commands.  Changes have been made to this  AE AA
	AE AA  release which may require changes to your configuration.  AE AA
	AE AA							     AE AA
	AE AA                To display the Release Notes,               AE AA
	AE AA               [B25BMU1]<sys>ReleaseNotes.doc,             AE AA
	AE AA							     AE AA
	AE AA             PRESS AEGOAA, otherwise PRESS AECANCELGOAA            AE AA
	AE AA							     AE AA
	AE							      AA

Type
[B25BMU1]<SYS>ReleaseNotes.doc
1
COPY
[kbd]
[VID]
CEF


	  AE							  AA
	  AE AA						         AE AA
	  AE AA     To Print the Release Notes (ReleaseNotes.Doc)    AE AA
	  AE AA    enter your Spooler Name in Square Brackets and    AE AA
	  AE AA                        PRESS AEGOAA                      AE AA
	  AE AA						         AE AA
	  AE AA     If you do not wish to print, PRESS AECANCELGOAA     AE AA
	  AE AA			 			         AE AA
	  AE						          AA


Copy
[B25BMU1]<SYS>ReleaseNotes.doc
1
copy
[kbd]
[vid]

PF
	
								
	  The Installation process will now update a loadable	
	  request file.  The default file is Request.Sys.	
	  If you are not booting the XE in Normal mode you	
	  may wish to change the name of the loadable request	
	  file below.						
								
	  Note  If you will be booting cluster workstations	
		  from this XE, you must update Request.Sys.	
		  You may need to perform this portion of the	
		  XESoftware Install routine a second time.	
								
	  Press AEGOAA when ready to continue...			
								
	
'
'  'Submit
'      File list          '[B25BMU1]<Sys>rqInstall.Sub
'      [Parameters]       '[Sys]<Sys>Request.Sys1
'      [Force Expansion?] 
'      [Show Expansion?]  
'   GO''
copy
[kbd]
[vid]

PF
	
								
	  The BMULTI Gateway is a software facility that	
	  enables BMULTI applications programs to communicate 	
	  with a host computer over a PollSelect line.	
		If you wish to install the BMULTI Gateway:	
								
			Press AEGOAA				
								
		Otherwise:					
								
			Press AECANCELAA AEGOAA				
								
	
'
'  'Submit
'      File list          '[B25BMU1]<Sys>BmInstall.Sub
'      [Parameters]       '0 1
'      [Force Expansion?] 'Yes1
'      [Show Expansion?]

COPY
[kbd]
[VID]
CEF
	
									
	  Installation of BMULTI Installation disk 1 of 3 completed. 	
	                                        			
	       Please INSERT BMULTI Installation disk 2 of 3		
				And PRESS  AAAEGOAA				
									
	

1
'
COPY
[kbd]
[VID]
CEF
	
								    
								    
	  The Line Monitor is a software facility that monitors    
	  and displays all line traffic as seen by BMULTI.  This   
	  will include restricted and proprietary data.            
								    
	  For security reasons, you may elect NOT to install the   
	  Line Monitor. Make sure that disk 2 of 3 is inserted.    
								    
		     Press AFGOAA to install the Line Monitor,          
		      or AFCANCELGOAA to skip installation.            
								    
	
'
Submit
[B25BMU2]<sys>InstallLineMonitor.sub
0 1
1


copy
[kbd]
[vid]

PF
	
								
	  The BMULTIX.25 Service is a software facility that	
	  provides an interface between BMULTI applications	
	  programs and the CTOS X.25 Gateway.			
								
	    If you wish to install the BMULTIX.25 Service:	
								
	       Make sure Installation Disk 2 is inserted and  
		    Press AEGOAA.					
								
		Otherwise:					
								
		    Press AFCANCELGOAA to skip installation.	
								
	
'
'  'Submit
'      File list          '[B25BMU2]<Sys>BmxInstall.Sub
'      [Parameters]       '0 1
'      [Force Expansion?] 'Yes1
'      [Show Expansion?]

COPY
[kbd]
[VID]
CEF
	
								    
	  The BMULTI Agent is a software facility that provides an 
	  interface between the CTOS MCS and the BMULTI Gateway,   
	  BMULTI SuspendResume Filter, or BMULTIX.25 Service.    
								    
	  The BMULTI Agent is only required by the CTOS MCS.       
								    
	    To Install the BMULTI Agent:                           
	       Make Sure That The Distribution Disk 3             
		       Is Inserted and Press AFGOAA.                    
								    
		Otherwise:					    
		    Press AFCANCELGOAA to skip installation.	    
								    
	'
'  'Submit
'      File list          '[B25BMU3]<Sys>InstallBmultiAgent.Sub
'      [Parameters]       '0 1
'      [Force Expansion?] 'Yes1
'      [Show Expansion?]

COPY
[kbd]
[VID]

CEF
	
								    
	  The BMULTI Suspend Resume filter allows two BMULTI       
	  applications to share the same session with the host.    
								    
	    To Install the BMULTI SuspendResume Filter:           
	       Make Sure That The Distribution Disk 3             
		       Is Inserted and Press AFGOAA.                    
								    
		Otherwise:					    
		    Press AFCANCELGOAA to skip installation.	    
								    
	
'
'  'Submit
'      File list          '[B25BMU3]<Sys>InstallBmSRFilter.Sub
'      [Parameters]       '0 1
'      [Force Expansion?] 'Yes1
'      [Show Expansion?]
'
Video
N
'
COPY
[kbd]
[VID]
PF

	     AE** BMULTI 10.4 Software Installation Complete **AA'
