'
Copy
[kbd]
[vid]
PF
               AIATTENTION:AA  AEINSTALLING THE XBIF SERVICEAA
        AEAA
        AE                                                               AA
        AE    Are you installing Standard Software on an EISAISA        AA
        AE    bus workstation (SG4000, SG6000 etc.)?                     AA
        AE                                                               AA
        AE    If your answer is YES, press AA<CANCELGO>AE now.              AA
        AE                                                               AA
        AE    If your answer is NO, press AA<GO>AE to continue.              AA
        AE                                                               AA
        AEAA
Install XBif Service1
Copy
[kbd]
[vid]
PF
              AMATTENTION:AA  SEQUENTIAL ACCESS SERVICE
        
                                                                       
           If [QIC] is not the first tape device on your system,       
           modify the [Device(s) ([QIC])] field of the command         
           form below  to include the additional tape device name.      
                                                                       
           For example, if you have a DDS tape drive and a QIC tape    
           drive, you must change this parameter to [DDS] [QIC].       
                                                                       
        

                             Press AE<GO>AA when ready.
Install Sequential Access Service
[QIC]1Submit
?0|0|0|[B25SID11]|<Sys>TapeInstall3.sub
0
ppy.user Tape.userDelete
Init.user Update.userDelete
XVTSignOn.runCopy
[kbd]
[vid]PF




        