vthlp3ObjIO version X2.4DATAFHt
vthlp3	tPetVT100 Function KeysPage 3 PPCTOS Key         Description1P	F1 to F10;Sends the user defined function key string for F1 to F10 orsends ESC [ xx  if no user defined sequence.(xx = 01 through 10)(Code_F1 to Code_F10<Sends the user defined function key string for F11 to F20 orsends ESC [ xx  if no user defined sequence.(xx = 11 through 20)(PShft_F1 to Shft_F10 Sends the user defined function key string for F21 to F30 orsends ESC [ xx  if no user defined sequence.(xx = 21 through 30)(P	Prev PageSends ESC [ 91  to host$	Next PageSends ESC [ 92  to host$	Scroll UpSends ESC [ 93  to host$Scroll Down	Sends ESC [ 94  to host$PPageSends ESC [ 81  to host$SentSends ESC [ 82  to host$LineSends ESC [ 83  to host$ColSends ESC [ 84  to host$ParaSends ESC [ 85  to host$WordSends ESC [ 86  to host$PPNote:   A carriage xreturn character is sent after the ESC sequence if so definedin the Vt100 Function Key configuration screen.t