'
?0
Video  yes
Type  [kbd]
  The Unisys datacomm installation diskette in [f0] contains the loadable
  request file Request.f.sys.  There are known request code conflicts when
  merging this file with CTOS [sys]<sys>Request.sys files.  This installation
  submit file will fix up the Request.f.sys file on the diskette so the
  conflict won't occur.  However, this will cause all the request codes in
  the 4000h range of Request.f.sys to overwrite those defined in your 
  [sys]<sys>Request.sys file.



	                AM                    Press  GO  when Ready                    
1AAPF
Delete  [scr]<$>*txt
List Request Set  [sys]<sys>request.sys  [scr]<$>request.txt
List Request Set  0  [scr]<$>request.f.tmp0
Run  [sys]<sys>FixRequestTxt.run  [scr]<$>request.f.tmp0  [scr]<$>request.f.tmp1  '40??h'  Version  3
Run  [sys]<sys>FixRequestTxt.run  [scr]<$>request.f.tmp1  [scr]<$>request.f.tmp2  '4076h'  Version  2
Run  [sys]<sys>FixRequestTxt.run  [scr]<$>request.f.tmp2  [scr]<$>request.f.tmp3  '4078h'  Version  2
Run  [sys]<sys>FixRequestTxt.run  [scr]<$>request.f.tmp3  [scr]<$>request.f.txt  '4080h'  Version  2
Make Request Set  [scr]<$>request*txt  [sys]<sys>request.sys
Type  [kbd]
  Because of request code conflicts, if you are installing this Unisys 
  product on a cluster workstation, the Request.f.sys file on [f0] must 
  also be merged on the master.  If you are doing this installation on a 
  cluster workstation, then press AMGOAA to merge [f0]<sys>request.f.sys on the 
  master, otherwise press AMCANCELAA and then AMGOAA.

  When the software installation is finished, you must reboot both the 
  master station and cluster workstations prior to running this product.


submit  [sys]<sys>FixRequestTxtM.sub1
Delete  [scr]<$>request*Z'
Z'
Z'Z'^Z'Z' (p (*(U1(J(ZJ(rJ(J(J(J(J(J([J(J(2(E(e((((	(
(oy)))3)O)p))