;THIS IS THE RAF CONFIGURATION FILE
;
;Only parameters mentioned in this file are configurable
;Any line starting with a semicolon is a comment line


;Source session Time Out Parameter
;It specifies the time out perion during a ViewControl session, if there was
;no activity on the source workstation
;Default 30 Minutes, minimum 1 Minute and Maximum 180 minutes
:SourceTimeOut:30

;Default value is the quote = 27 hex or 39 decimal.
:ActionQuote:39

;RS232 Timeout period
;This parameter specifies how many seconds RS232 SourceTarget Interface should
;wait for each other without getting any message before disconnecting
;
;NOTE: If the Target is a BNET Target then this time out value should be 
;      greater that the BNet timeout else the session can terminate sometimes.
;      To calculate the timeout use the formula TIMEOUT = X * 6 + 10
;      Where TIMIOUT = Timeout period in seconds
;            X       = the value specified below.
;
;NOTE: If your RS232 Session terminates abnormally (i.e. ACTION+FINISH etc. ) 
;      then you must wait for TIMEOUT seconds before retrying another session
;      with that target. This will allow the target to reset properly and be
;      ready for your next transmission.
;
;Default 10 sec, minimum 6 sec, Maximum 60 Secs
:RS232TimeOut:10

;Timeout for transmitting keys from source to the target in a block
;Default is 3 Sec, minimum 2 sec and maximum 10 sec
:BlockKeysTimeout:3

;Number of Send Key requests to keep pending
;
;NOTE: Higher number of requests can boost performance in some cases, but
;      they also load your system. You can decide what is best for your 
;      configuration.
;
;default 2, minimum 2, maximum 5
:NoOfSendKeys:2

;Video Update buffer size parameter
;default 1024, minimum 500 and maximum 1024 bytes
:SzVidUpdateBuffer:1024

;Notification Parameter
;Default No, allowed values are Audio, Visual, None
:Notification:No


;Visual Notification Blinking Parameter, Used if Visual notification
;Default No, allowed values are Yes for blinking notification, No otherwise
:NotifyBlink:No

;Target Security Parameter
;Default no, permitted values are Yes and No
;Using this parameter will override the target security in the RAF Profiles
;Disabled this parameter. 
;TargetSecurity:No

;Wrap Log File Allowed parameter
;Default Yes, permitted values are Yes and No
:WrapLogFileAllowed:Yes

