
*************************************************************************
*************************************************************************
**                                                                     **
**   Application notes for Zilog Microcontrollers (informal document)  **
**                                                                     **
**    To find the application notes for your device search for the     **
**    'core' part name.  As an example the Z86E3016 28 pin SOIC can    **
**    be found if you search using just "86E30". (without the quotes)  **
**                                                                     **
*************************************************************************
*************************************************************************


*************************************************************************

 86E3016
 --------

 *----------------- Programmable OTP Options ---------------------------*

 To setup for programming the "Programmable OTP Options" you must
 set the requied bits in User RAM at address location 1000 hex.

 Format of the Programmable OTP Options Byte:

 Bit 7 = "Don't Care"
 Bit 6 = "Don't Care"
 Bit 5 = Crystal Oscillator Feedback Resistor Disable
 Bit 4 = Permanently Enabled WDT
 Bit 3 = Auto Latch Disable
 Bit 2 = RC Oscillator
 Bit 1 = RAM Protect
 Bit 0 = "Don't Care" bit; see below to program Protection

 To program the "Programmable OTP Options" in TaskLink you
 must set the Special Data #1 flag to Y.

 To program the "Programmable OTP Options" in Terminal mode
 set the "Program Configuration" flag to Y.

 *-------------------- EPROM Protect ----------------------------------*

 Programming the EPROM Protect feature of the device requires the
 "Security fuse" flag must be enabled during a  progamming operation.

************************************************************************
