;****************************** MODULE HEADER ********************************;
;*                                                                           *;
;* UNISYS BELIEVES THAT THE SOFTWARE FURNISHED HEREWITH IS ACCURATE AND      *;
;* RELIABLE, AND MUCH CARE HAS BEEN TAKEN IN ITS PREPARATION.  HOWEVER,      *;
;* NO RESPONSIBILITY, FINANCIAL OR OTHERWISE, CAN BE ACCEPTED FOR ANY        *;
;* CONSEQUENCES ARISING OUT OF THE USE OF THIS MATERIAL, INCLUDING LOSS OF   *;
;* PROFIT, INDIRECT, SPECIAL, OR CONSEQUENTIAL DAMAGES, THERE ARE NO         *;
;* WARRANTIES WHICH EXTEND BEYOND THE PROGRAM SPECIFICATION.                 *;
;*                                                                           *;
;* THE CUSTOMER SHOULD EXERCISE CARE TO ASSURE THAT USE OF THE SOFTWARE      *;
;* WILL BE IN FULL COMPLIANCE WITH LAWS, RULES AND REGULATIONS OF THE        *;
;* JURISDICTIONS WITH RESPECT TO WHICH IT IS USED.                           *;
;*                                                                           *;
;*                                                                           *;
;* ************************* END OF MODULE HEADER ************************** *;


; Supergen System Volume  No password protection or Encryption

:FormatTemplate:SgenSysVolume
:MaxFilesOnVolume:
:PrimaryFileHeadersOnly?:
:MaxDirectories:
:MaxFilesInSysDirectory:
:PasswordEncryption?:
:Debug?:
:SysDirectoryPassword:
:ProtectSysDirectory?:
:SystemImageSize:1280
:CrashFileSize:8192
:SystemLogFileSize:48
:SuppressFormat?:No
:SurfaceTestsIfUnformatted:1
:SurfaceTestsIfFormatted:1
:OldCTOSFormat?:No
:SuppressVolumeStructures?:No


; Supergen System Volume  Encrypted password protection

:FormatTemplate:SgenSysVolumeEncrypt
:MaxFilesOnVolume:
:PrimaryFileHeadersOnly?:
:MaxDirectories:
:MaxFilesInSysDirectory:
:PasswordEncryption?:Yes
:Debug?:
:SysDirectoryPassword:Sys
:ProtectSysDirectory?:Yes
:SystemImageSize:1280
:CrashFileSize:8192
:SystemLogFileSize:48
:SuppressFormat?:No
:SurfaceTestsIfUnformatted:1
:SurfaceTestsIfFormatted:1
:OldCTOSFormat?:No
:SuppressVolumeStructures?:No


; Supergen System Volume  NonEncrypted password protection

:FormatTemplate:SgenSysVolumeProtect
:MaxFilesOnVolume:
:PrimaryFileHeadersOnly?:
:MaxDirectories:
:MaxFilesInSysDirectory:
:PasswordEncryption?:
:Debug?:
:SysDirectoryPassword:Sys
:ProtectSysDirectory?:Yes
:SystemImageSize:1280
:CrashFileSize:8192
:SystemLogFileSize:48
:SuppressFormat?:No
:SurfaceTestsIfUnformatted:1
:SurfaceTestsIfFormatted:1
:OldCTOSFormat?:No
:SuppressVolumeStructures?:No


; Sgen System Volume Save Non CTOS partition Encrypted password protection

:FormatTemplate:SgenSavePartitionEncrypt
:MaxFilesOnVolume:
:PrimaryFileHeadersOnly?:
:MaxDirectories:
:MaxFilesInSysDirectory:
:PasswordEncryption?:Yes
:Debug?:
:SysDirectoryPassword:Sys
:ProtectSysDirectory?:Yes
:SystemImageSize:1280
:CrashFileSize:8192
:SystemLogFileSize:48
:SuppressFormat?:Yes
:SurfaceTestsIfUnformatted:1
:SurfaceTestsIfFormatted:1
:OldCTOSFormat?:No
:SuppressVolumeStructures?:No


; Sgen System Volume Save Non CTOS partition NonEncrypted password protection

:FormatTemplate:SgenSavePartitionProtect
:MaxFilesOnVolume:
:PrimaryFileHeadersOnly?:
:MaxDirectories:
:MaxFilesInSysDirectory:
:PasswordEncryption?:
:Debug?:
:SysDirectoryPassword:Sys
:ProtectSysDirectory?:Yes
:SystemImageSize:1280
:CrashFileSize:8192
:SystemLogFileSize:48
:SuppressFormat?:Yes
:SurfaceTestsIfUnformatted:1
:SurfaceTestsIfFormatted:1
:OldCTOSFormat?:No
:SuppressVolumeStructures?:No


; Sgen System Volume Save Non CTOS partition No password protection or  
  Encryption

:FormatTemplate:SgenSavePartition
:MaxFilesOnVolume:
:PrimaryFileHeadersOnly?:
:MaxDirectories:
:MaxFilesInSysDirectory:
:PasswordEncryption?:
:Debug?:
:SysDirectoryPassword:
:ProtectSysDirectory?:
:SystemImageSize:1280
:CrashFileSize:8192
:SystemLogFileSize:48
:SuppressFormat?:Yes
:SurfaceTestsIfUnformatted:1
:SurfaceTestsIfFormatted:1
:OldCTOSFormat?:No
:SuppressVolumeStructures?:No

; Ngen Workstation System Volume  NonEncrypted password protection

:FormatTemplate:WSSysVolumeProtect
:MaxFilesOnVolume:
:PrimaryFileHeadersOnly?:
:MaxDirectories:
:MaxFilesInSysDirectory:
:PasswordEncryption?:
:Debug?:
:SysDirectoryPassword:Sys
:ProtectSysDirectory?:Yes
:SystemImageSize:1024
:CrashFileSize:2048
:SystemLogFileSize:48
:SuppressFormat?:No
:SurfaceTestsIfUnformatted:4
:SurfaceTestsIfFormatted:1
:OldCTOSFormat?:Yes


; Ngen Workstation System Volume  No password protection or Encryption

:FormatTemplate:WSSysVolume
:MaxFilesOnVolume:
:PrimaryFileHeadersOnly?:
:MaxDirectories:
:MaxFilesInSysDirectory:
:PasswordEncryption?:
:Debug?:
:SysDirectoryPassword:
:ProtectSysDirectory?:
:SystemImageSize:1024
:CrashFileSize:2048
:SystemLogFileSize:48
:SuppressFormat?:No
:SurfaceTestsIfUnformatted:4
:SurfaceTestsIfFormatted:1
:OldCTOSFormat?:Yes


; Data Volume (WS or SRP)  No password protection or Encryption
:FormatTemplate:DataVolume
:MaxFilesOnVolume:
:PrimaryFileHeadersOnly?:
:MaxDirectories:
:MaxFilesInSysDirectory:
:PasswordEncryption?:
:Debug?:
:SysDirectoryPassword:
:ProtectSysDirectory?:
:SystemImageSize:0
:CrashFileSize:0
:SystemLogFileSize:0
:SuppressFormat?:no
:SurfaceTestsIfUnformatted:4
:SurfaceTestsIfFormatted:1
:OldCTOSFormat?:Yes


; Small Data Volume (WS or SRP)  No password protection or Encryption
; Limits number of files to 500

:FormatTemplate:SmallDataVolume
:MaxFilesOnVolume:500
:PrimaryFileHeadersOnly?:
:MaxDirectories:
:MaxFilesInSysDirectory:
:PasswordEncryption?:
:Debug?:
:Verify?:no
:SysDirectoryPassword:
:ProtectSysDirectory?:
:SystemImageSize:0
:CrashFileSize:0
:SystemLogFileSize:0
:SuppressFormat?:No
:SurfaceTestsIfUnformatted:4
:SurfaceTestsIfFormatted:1
:OldCTOSFormat?:Yes


; Default Hard Disk (St506, SMD or SCSI) on WS or SRP
; Used if no FormatTemplate is specified in the parameter list

:FormatTemplate:DiskDefault
:MaxFilesOnVolume:
:PrimaryFileHeadersOnly?:no
:MaxDirectories:
:MaxFilesInSysDirectory:
:PasswordEncryption?:
:Debug?:
:SysDirectoryPassword:
:ProtectSysDirectory?:
:SystemImageSize:1280
:CrashFileSize:2048
:SystemLogFileSize:48
:SuppressFormat?:No
:SurfaceTestsIfUnformatted:4
:SurfaceTestsIfFormatted:1
:OldCTOSFormat?:Yes


; Default Floppy on Workstation
; Used if no FormatTemplate is specified in the parameter list

:FormatTemplate:FloppyDefault
:MaxFilesOnVolume:
:PrimaryFileHeadersOnly?:yes
:MaxDirectories:
:MaxFilesInSysDirectory:
:PasswordEncryption?:
:Debug?:
:SysDirectoryPassword:
:ProtectSysDirectory?:
:SystemImageSize:0
:CrashFileSize:0
:SystemLogFileSize:0
:SuppressFormat?:No
:SurfaceTestsIfUnformatted:1
:SurfaceTestsIfFormatted:1
:OldCTOSFormat?:Yes


; Protected Floppy   NonEncrypted password protection

:FormatTemplate:FloppyProtect
:MaxFilesOnVolume:60
:PrimaryFileHeadersOnly?:no
:MaxDirectories:
:MaxFilesInSysDirectory:12
:PasswordEncryption?:no
:Debug?:
:SysDirectoryPassword:sys
:ProtectSysDirectory?:yes
:SystemImageSize:0
:CrashFileSize:0
:SystemLogFileSize:0
:SuppressFormat?:No
:SurfaceTestsIfUnformatted:1
:SurfaceTestsIfFormatted:1
:OldCTOSFormat?:Yes


; Archival Floppy   No password protection or Encryption
; Minimal volume structures so that the most data can be written to it.

:FormatTemplate:FloppyArchive
:MaxFilesOnVolume:12
:PrimaryFileHeadersOnly?:
:MaxDirectories:2
:MaxFilesInSysDirectory:10
:PasswordEncryption?:
:Debug?:
:SysDirectoryPassword:
:ProtectSysDirectory?:
:SystemImageSize:0
:CrashFileSize:0
:SystemLogFileSize:0
:SuppressFormat?:No
:SurfaceTestsIfUnformatted:1
:SurfaceTestsIfFormatted:1
:OldCTOSFormat?:Yes


; Data Floppy   No password protection or Encryption

:FormatTemplate:FloppyData
:MaxFilesOnVolume:60
:PrimaryFileHeadersOnly?:
:MaxDirectories:
:MaxFilesInSysDirectory:12
:PasswordEncryption?:
:Debug?:
:SysDirectoryPassword:
:ProtectSysDirectory?:
:SystemImageSize:0
:CrashFileSize:0
:SystemLogFileSize:0
:SuppressFormat?:No
:SurfaceTestsIfUnformatted:1
:SurfaceTestsIfFormatted:1
:OldCTOSFormat?:Yes

; Used by CreateBackupFloppy.Sub   No password protection or Encryption
; This is the boot diskette.

:FormatTemplate:CreateBackupFloppySys
:MaxFilesOnVolume:20
:PrimaryFileHeadersOnly?:Yes
:MaxDirectories:1
:MaxFilesInSysDirectory:
:PasswordEncryption?:
:Debug?:
:SysDirectoryPassword:
:ProtectSysDirectory?:
:SystemImageSize:640
:CrashFileSize:0
:SystemLogFileSize:0
:SuppressFormat?:No
:SurfaceTestsIfUnformatted:1
:SurfaceTestsIfFormatted:1
:OldCTOSFormat?:Yes


; Used by CreateBackupFloppy.Sub   No password protection or Encryption
; This is the continuation diskette.

:FormatTemplate:CreateBackupFloppyContinue
:MaxFilesOnVolume:20
:PrimaryFileHeadersOnly?:Yes
:MaxDirectories:1
:MaxFilesInSysDirectory:
:PasswordEncryption?:
:Debug?:
:SysDirectoryPassword:
:ProtectSysDirectory?:
:SystemImageSize:0
:CrashFileSize:0
:SystemLogFileSize:0
:SuppressFormat?:No
:SurfaceTestsIfUnformatted:1
:SurfaceTestsIfFormatted:1
:OldCTOSFormat?:Yes

; SRP SCSI System Volume  No password protection or Encryption

:FormatTemplate:SrpScsiSysVolume
:MaxFilesOnVolume:
:PrimaryFileHeadersOnly?:
:MaxDirectories:
:MaxFilesInSysDirectory:
:PasswordEncryption?:
:Debug?:
:SysDirectoryPassword:
:ProtectSysDirectory?:
:SystemImageSize:1152
:CrashFileSize:8192
:SystemLogFileSize:64
:SuppressFormat?:no
:SurfaceTestsIfUnformatted:4
:SurfaceTestsIfFormatted:1
:OldCTOSFormat?:No


; SRP SCSI System Volume  NonEncrypted password protection

:FormatTemplate:SrpScsiSysVolumeProtect
:MaxFilesOnVolume:
:PrimaryFileHeadersOnly?:
:MaxDirectories:
:MaxFilesInSysDirectory:
:PasswordEncryption?:
:Debug?:
:SysDirectoryPassword:Sys
:ProtectSysDirectory?:Yes
:SystemImageSize:1152
:CrashFileSize:8192
:SystemLogFileSize:64
:SuppressFormat?:no
:SurfaceTestsIfUnformatted:4
:SurfaceTestsIfFormatted:1
:OldCTOSFormat?:No


; SRP SCSI System Volume  Encrypted password protection

:FormatTemplate:SrpScsiSysVolumeEncrypt
:MaxFilesOnVolume:
:PrimaryFileHeadersOnly?:
:MaxDirectories:
:MaxFilesInSysDirectory:
:PasswordEncryption?:Yes
:Debug?:
:SysDirectoryPassword:Sys
:ProtectSysDirectory?:Yes
:SystemImageSize:1152
:CrashFileSize:8192
:SystemLogFileSize:64
:SuppressFormat?:no
:SurfaceTestsIfUnformatted:4
:SurfaceTestsIfFormatted:1
:OldCTOSFormat?:No


; SRP Winchester (ST506) System Volume  No password protection or Encryption

:FormatTemplate:SrpWinSysVolume
:MaxFilesOnVolume:
:PrimaryFileHeadersOnly?:
:MaxDirectories:
:MaxFilesInSysDirectory:
:PasswordEncryption?:
:Debug?:
:SysDirectoryPassword:
:ProtectSysDirectory?:
:SystemImageSize:1152
:CrashFileSize:1536
:SystemLogFileSize:32
:SuppressFormat?:no
:SurfaceTestsIfUnformatted:4
:SurfaceTestsIfFormatted:1
:OldCTOSFormat?:No


; SRP Winchester (ST506) System Volume  NonEncrypted password protection

:FormatTemplate:SrpWinSysVolumeProtect
:MaxFilesOnVolume:
:PrimaryFileHeadersOnly?:
:MaxDirectories:
:MaxFilesInSysDirectory:
:PasswordEncryption?:
:Debug?:
:SysDirectoryPassword:Sys
:ProtectSysDirectory?:Yes
:SystemImageSize:1152
:CrashFileSize:1536
:SystemLogFileSize:32
:SuppressFormat?:no
:SurfaceTestsIfUnformatted:4
:SurfaceTestsIfFormatted:1
:OldCTOSFormat?:No


; SRP Winchester (ST506) System Volume  Encrypted password protection

:FormatTemplate:SrpWinSysVolumeEncrypt
:MaxFilesOnVolume:
:PrimaryFileHeadersOnly?:
:MaxDirectories:
:MaxFilesInSysDirectory:
:PasswordEncryption?:Yes
:Debug?:
:SysDirectoryPassword:Sys
:ProtectSysDirectory?:Yes
:SystemImageSize:1152
:CrashFileSize:1536
:SystemLogFileSize:32
:SuppressFormat?:no
:SurfaceTestsIfUnformatted:4
:SurfaceTestsIfFormatted:1
:OldCTOSFormat?:No


; SRP SMD System Volume  No password protection or Encryption

:FormatTemplate:SrpSMDSysVolume
:MaxFilesOnVolume:
:PrimaryFileHeadersOnly?:
:MaxDirectories:
:MaxFilesInSysDirectory:
:PasswordEncryption?:
:Debug?:
:SysDirectoryPassword:
:ProtectSysDirectory?:
:SystemImageSize:1152
:CrashFileSize:1536
:SystemLogFileSize:32
:SuppressFormat?:no
:SurfaceTestsIfUnformatted:4
:SurfaceTestsIfFormatted:1
:OldCTOSFormat?:No


; SRP SMD System Volume  NonEncrypted password protection

:FormatTemplate:SrpSMDSysVolumeProtect
:MaxFilesOnVolume:
:PrimaryFileHeadersOnly?:
:MaxDirectories:
:MaxFilesInSysDirectory:
:PasswordEncryption?:
:Debug?:
:SysDirectoryPassword:Sys
:ProtectSysDirectory?:Yes
:SystemImageSize:1152
:CrashFileSize:1536
:SystemLogFileSize:32
:SuppressFormat?:no
:SurfaceTestsIfUnformatted:4
:SurfaceTestsIfFormatted:1
:OldCTOSFormat?:No


; SRP SMD System Volume  Encrypted password protection

:FormatTemplate:SrpSMDSysVolumeEncrypt
:MaxFilesOnVolume:
:PrimaryFileHeadersOnly?:
:MaxDirectories:
:MaxFilesInSysDirectory:
:PasswordEncryption?:Yes
:Debug?:
:SysDirectoryPassword:Sys
:ProtectSysDirectory?:Yes
:SystemImageSize:1152
:CrashFileSize:1536
:SystemLogFileSize:32
:SuppressFormat?:no
:SurfaceTestsIfUnformatted:4
:SurfaceTestsIfFormatted:1
:OldCTOSFormat?:No


; SRP SMD Data Volume  No password protection or Encryption

:FormatTemplate:SrpDataVolume
:MaxFilesOnVolume:
:PrimaryFileHeadersOnly?:
:MaxDirectories:
:MaxFilesInSysDirectory:
:PasswordEncryption?:
:Debug?:
:SysDirectoryPassword:
:ProtectSysDirectory?:
:SystemImageSize:0
:CrashFileSize:0
:SystemLogFileSize:0
:SuppressFormat?:yes
:SurfaceTestsIfUnformatted:4
:SurfaceTestsIfFormatted:1
:OldCTOSFormat?:No




; Default Floppy DeviceTemplate

:DeviceTemplate:FloppyType
:CylindersPerDisk:
:TracksPerCylinder:
:SectorsPerTrack:
:BytesPerSector:512
:Removable?:Yes
:HiCapacityFloppy?:No


; High Capacity Floppy
; (Nec controller  286i, 386i, B39, HSD040, MS5 and MS6)
; This doubles the capacity of the floppy.
; You must use the High Density (AT compatible) Floppy disks.

:DeviceTemplate:FloppyTypeHiCap
:Removable?:Yes
:HiCapacityFloppy?:Yes



* Workstation only Drive types *
* Use the Drive type letter on the bottom of the disk drive. *

; ACER 3.5 40Mb

:DeviceTemplate:ACER40
:CylindersPerDisk:977
:TracksPerCylinder:5
:SectorsPerTrack:17
:BytesPerSector:512
:UtilizeEcc?:Yes

; Connor 2.5 64Mb 

:DeviceTemplate:CP2064
:CylindersPerDisk:823
:TracksPerCylinder:4
:SectorsPerTrack:38
:BytesPerSector:512
:UtilizeEcc?:Yes

; 10 Meg HardFloppy disks

:DeviceTemplate:A
:CylindersPerDisk:306
:TracksPerCylinder:4
:SectorsPerTrack:16
:BytesPerSector:512
:UtilizeEcc?:no


; 40 Meg Hard disks

:DeviceTemplate:A1
:CylindersPerDisk:977
:TracksPerCylinder:5
:SectorsPerTrack:16
:BytesPerSector:512
:UtilizeEcc?:Yes


; 10 Meg HardFloppy disks

:DeviceTemplate:B
:CylindersPerDisk:306
:TracksPerCylinder:4
:SectorsPerTrack:16
:BytesPerSector:512
:UtilizeEcc?:no


; 20 Meg HardFloppy disks

* BTOS ONLY *
:DeviceTemplate:C
:CylindersPerDisk:612
:TracksPerCylinder:4
:SectorsPerTrack:16
:BytesPerSector:512
:UtilizeEcc?:no


; 40 Meg Hard disks

:DeviceTemplate:D
:CylindersPerDisk:645
:TracksPerCylinder:7
:SectorsPerTrack:16
:BytesPerSector:512
:UtilizeEcc?:no


; 32 Meg Hard disks

:DeviceTemplate:E
:CylindersPerDisk:512
:TracksPerCylinder:8
:SectorsPerTrack:16
:BytesPerSector:512
:UtilizeEcc?:no


; 20 Meg HardFloppy disks

:DeviceTemplate:F
:CylindersPerDisk:612
:TracksPerCylinder:4
:SectorsPerTrack:16
:BytesPerSector:512
:UtilizeEcc?:no


; 20 Meg HardFloppy disks

:DeviceTemplate:G
:CylindersPerDisk:612
:TracksPerCylinder:4
:SectorsPerTrack:16
:BytesPerSector:512
:UtilizeEcc?:no


; 56.5 Meg Hard disks

:DeviceTemplate:H
:CylindersPerDisk:987
:TracksPerCylinder:7
:SectorsPerTrack:16
:BytesPerSector:512
:UtilizeEcc?:no


; 67 Meg Hard disks

:DeviceTemplate:J
:CylindersPerDisk:1024
:TracksPerCylinder:8
:SectorsPerTrack:16
:BytesPerSector:512
:UtilizeEcc?:no


; 67 Meg Hard disks

:DeviceTemplate:K
:CylindersPerDisk:1024
:TracksPerCylinder:8
:SectorsPerTrack:16
:BytesPerSector:512
:UtilizeEcc?:yes


; 67 Meg Hard disks

:DeviceTemplate:L
:CylindersPerDisk:1166
:TracksPerCylinder:7
:SectorsPerTrack:16
:BytesPerSector:512
:UtilizeEcc?:no


; 67 Meg Hard disks

:DeviceTemplate:M
:CylindersPerDisk:1024
:TracksPerCylinder:8
:SectorsPerTrack:16
:BytesPerSector:512
:UtilizeEcc?:no


; 40 Meg Hard disks

* BTOS Only *
:DeviceTemplate:N
:CylindersPerDisk:699
:TracksPerCylinder:7
:SectorsPerTrack:16
:BytesPerSector:512
:UtilizeEcc?:no


; 68 Meg Hard disks (Ecc)

* BTOS Only *
:DeviceTemplate:O
:CylindersPerDisk:830
:TracksPerCylinder:10
:SectorsPerTrack:16
:BytesPerSector:512
:UtilizeEcc?:yes



; 40 Meg Hard disks (Ecc)

* BTOS Only *
:DeviceTemplate:P
:CylindersPerDisk:989
:TracksPerCylinder:5
:SectorsPerTrack:16
:BytesPerSector:512
:UtilizeEcc?:yes


; 80 Meg Hard disks

:DeviceTemplate:Q
:CylindersPerDisk:823
:TracksPerCylinder:5
:SectorsPerTrack:38
:BytesPerSector:512
:UtilizeEcc?:no


; 53 Meg Hard disks

:DeviceTemplate:R
:CylindersPerDisk:823
:TracksPerCylinder:6
:SectorsPerTrack:21
:BytesPerSector:512
:UtilizeEcc?:no


; 21 Meg Hard disks

:DeviceTemplate:S
:CylindersPerDisk:613
:TracksPerCylinder:4
:SectorsPerTrack:17
:BytesPerSector:512
:UtilizeEcc?:no

; 40 Meg Hard disks

:DeviceTemplate:V
:CylindersPerDisk:834
:TracksPerCylinder:3
:SectorsPerTrack:32
:BytesPerSector:512
:UtilizeEcc?:no



* XESRP only Drive types *

; Atasi 46 Meg (St506)

:DeviceTemplate:Atasi46
:CylindersPerDisk:645
:TracksPerCylinder:7
:SectorsPerTrack:17
:BytesPerSector:512
:WritePreCompCyl:320
:SeekStepRate:14


; Ball 100 Meg (St506)

:DeviceTemplate:Ball100
:CylindersPerDisk:1024
:TracksPerCylinder:5
:SectorsPerTrack:32
:BytesPerSector:512
:Removable?:Yes
:SeekStepRate:14


; CDC 300 Meg (SMD)

:DeviceTemplate:CDC300
:CylindersPerDisk:823
:TracksPerCylinder:19
:SectorsPerTrack:32
:BytesPerSector:512
:Removable?:Yes


; CDC 340 Meg (SMD)

:DeviceTemplate:CDC340
:CylindersPerDisk:711
:TracksPerCylinder:24
:SectorsPerTrack:32
:BytesPerSector:512
:Removable?:No


; CDC 675 Meg (SMD)

:DeviceTemplate:CDC675
:CylindersPerDisk:840
:TracksPerCylinder:40
:SectorsPerTrack:32
:BytesPerSector:512
:Removable?:No


; Fujitsu 80 Meg (St506)

:DeviceTemplate:Fujitsu80
:CylindersPerDisk:589
:TracksPerCylinder:7
:SectorsPerTrack:32
:BytesPerSector:512
:Removable?:No
:SeekStepRate:14


; Hitachi 51 Meg (St506)

:DeviceTemplate:Hitachi51
:CylindersPerDisk:699
:TracksPerCylinder:7
:SectorsPerTrack:16
:BytesPerSector:512
:Removable?:No
:WritePreCompCyl:256
:SeekStepRate:14


; Hitachi 85 Meg (St506)

:DeviceTemplate:Hitachi85
:CylindersPerDisk:823
:TracksPerCylinder:10
:SectorsPerTrack:16
:BytesPerSector:512
:Removable?:No
:SeekStepRate:14


; Maxtor 53 Meg (St506)

:DeviceTemplate:Maxtor53
:CylindersPerDisk:903
:TracksPerCylinder:5
:SectorsPerTrack:17
:BytesPerSector:512
:Removable?:No
:SeekStepRate:14


; Maxtor 143 Meg (St506)

:DeviceTemplate:Maxtor143
:CylindersPerDisk:918
:TracksPerCylinder:15
:SectorsPerTrack:17
:BytesPerSector:512
:Removable?:No
:SeekStepRate:14


; Memorex 166 Meg (SMD)

:DeviceTemplate:Memorex166
:CylindersPerDisk:823
:TracksPerCylinder:10
:SectorsPerTrack:32
:BytesPerSector:512
:Removable?:No


; Micropolis 52 Meg (St506)

:DeviceTemplate:Micropolis52
:CylindersPerDisk:753
:TracksPerCylinder:6
:SectorsPerTrack:16
:BytesPerSector:512
:Removable?:No
:SeekStepRate:14


; Micropolis 85 Meg (St506)

:DeviceTemplate:Micropolis85
:CylindersPerDisk:1024
:TracksPerCylinder:8
:SectorsPerTrack:17
:BytesPerSector:512
:Removable?:No
:SeekStepRate:14


; Nortel 350 Meg (SMD)

:DeviceTemplate:Nortel350
:CylindersPerDisk:1332
:TracksPerCylinder:12
:SectorsPerTrack:33
:BytesPerSector:512
:SpiralFactor:4
:Removable?:No


; Toshiba 85 Meg (St506)

:DeviceTemplate:Toshiba85
:CylindersPerDisk:830
:TracksPerCylinder:10
:SectorsPerTrack:17
:BytesPerSector:512
:Removable?:No
:WritePreCompCyl:512
:SeekStepRate:14


; Unknown Disk type 
; Used if the disk type can not be determined by the hardware.

:DeviceTemplate:Unknown
:CylindersPerDisk:300
:TracksPerCylinder:7
:SectorsPerTrack:16
:BytesPerSector:512
:Removable?:No


; SCSI Disk type 

:DeviceTemplate:ScsiType
:BytesPerSector:512


; SRP 1 Meg Memory disk Format Template  Used for creating Boot tapes

:FormatTemplate:MemDisk1
:MaxFilesOnVolume:30
:PrimaryFileHeadersOnly?:Y
:MaxDirectories:1
:MaxFilesInSysDirectory:20
:PasswordEncryption?:
:Debug?:
:SysDirectoryPassword:
:ProtectSysDirectory?:
:SystemImageSize:0
:CrashFileSize:0
:SystemLogFileSize:4
:SuppressFormat?:no
:SurfaceTestsIfUnformatted:0
:SurfaceTestsIfFormatted:0
:OldCTOSFormat?:No


; SRP 1 Meg Memory disk Device Template  Used for creating Boot tapes

:DeviceTemplate:MemDisk1
:BytesPerSector:512
:BlocksPerDisk:2304


; SRP 3 Meg Memory disk Format Template  Used for creating Boot tapes

:FormatTemplate:MemDisk3
:MaxFilesOnVolume:50
:PrimaryFileHeadersOnly?:Y
:MaxDirectories:1
:MaxFilesInSysDirectory:50
:PasswordEncryption?:
:Debug?:
:SysDirectoryPassword:
:ProtectSysDirectory?:
:SystemImageSize:0
:CrashFileSize:0
:SystemLogFileSize:4
:SuppressFormat?:no
:SurfaceTestsIfUnformatted:0
:SurfaceTestsIfFormatted:0
:OldCTOSFormat?:No


; SRP 3 Meg Memory disk Device Template  Used for creating Boot tapes

:DeviceTemplate:MemDisk3
:BytesPerSector:512
:BlocksPerDisk:6144
c?:no


; 67 Meg Hard disks

:DeviceTemplate:M
:CylindersPerDisk:10