'
' Install OS <Gen> directory
' Copy files from [F0]<Gen> to the <Gen> directory of the logged in volume
'
Type
[Kbd]PF

Modify the following Path command as follows:

	1)  Supply the volume name where you wish to build the OS.
	2)  Supply the volume password for that volume (if one exists).

Press GO when ready.Path

Gen1Type
[Kbd]PFCreate Directory
'[New directory name]                    '<Gen>
'[Default protection level (default 15)] '
'[Default number of files (default 45)]  '400
'[Password for new directory]            '
'[Volume password]                       '
'
' copy the files
'
LCopy
'File List              '[F0]<Gen>*
'[File prefix(s) from]  '
'[File prefix(s) to]    '<Gen>
'[File suffix(s)]       '
'[Overwrite OK?]        'y
'[Confirm each?]        '
'[Continue on error?]   '
'[Verify copy?]         'y
LCopy
'File List              '[f0]<sys>LinkCtos.sub
'[File prefix(s) from]  '
'[File prefix(s) to]    '[sys]<sys>
'[File suffix(s)]       '
'[Overwrite OK?]        'y
'[Confirm each?]        '
'[Continue on error?]   '
'[Verify copy?]         'y
Submit
'File List        '[f0]<sys>LinkCtosCmd.sub 
'[Parameters]     '
'[ForceExpansion] '
'[Show Expansion] '
Type
[kbd]
PF
Remove the diskette from the floppy drive [f0] and insert the
CTOS Build diskette 2 of 3.





INSERT DISK 2:  AB                    Press  GO  when Ready                    
1AAEF
LCopy
'File List              '[F0]<Gen>*
'[File prefix(s) from]  '
'[File prefix(s) to]    '<Gen>
'[File suffix(s)]       '
'[Overwrite OK?]        'y
'[Confirm each?]        '
'[Continue on error?]   '
'[Verify copy?]         'yType
[kbd]
PF
Remove the diskette from the floppy drive [f0] and insert the
CTOS Build diskette 3 of 3.





INSERT DISK 3:  AB                    Press  GO  when Ready                    
1AAEF
LCopy
'File List              '[F0]<Gen>*
'[File prefix(s) from]  '
'[File prefix(s) to]    '<Gen>
'[File suffix(s)]       '
'[Overwrite OK?]        'y
'[Confirm each?]        '
'[Continue on error?]   '
'[Verify copy?]         'y
Type
[Kbd]

  In order to build a customized version of CTOS you need the Software
  Development utilities.  If you have not yet done so, insert the 
  SOFTWARE DEVELOPMENT diskettes and give the following command:

	Install   <GO>

