
Diagnostic control program (CP) on disk 1 of 6
CWS Workstations

	CM002	512 Kb processor
	CM003	1 Mb processor
	NGEN Modules	Description	BTOS Modules

	CP0018	8 Mhz 80186 processor	B26CPU
	no equiv	Hardware ID option	B25HIAHID
	KM001	Keyboard 	B25K1
	no equiv	K2, K4, K3K5 Keyboards	B25K2K3K4K5
	no equiv	2 button Mouse	B25MOU
	PD001	3 button Mouse	B25MO3


Disk diagnostic control program (DCP) on disk 2 of 6
	NGEN Modules	Description	BTOS Modules

	no equiv	single floppy disk	B25M0
	FD001	dual floppy disk	no equiv
	FD0A1	dual floppy disk	B25M1
	HD002	10 Mb HD wfloppy	B25M3
	HD003	20 Mb HD wfloppy	no equiv
	HD0A3	20 Mb HD wfloppy	B25M4
	HD006	20 Mb hard disk upgrade	no equiv
	HD011	32 Mb hard disk upgrade	no equiv
	HD020	85 Mb hard disk upgrade	no equiv
	no equiv	40 Mb HD wfloppy	B25M5
	HD010	40 Mb hard disk upgrade	no equiv
	HX002	10 Mb hard disk expansion	B25MX3
	HX003	20 Mb hard disk expansion	B25MX4
	HX011	32 Mb hard disk expansion	B25MX5
	HX020	85 Mb hard disk expansion	B25MX6
	HB001	tape backup	no equiv
	no equiv	tape backup	B25TS
	no equiv	all HD wfloppy	B25Mx
	no equiv	all ECC HD upgrades	B25MCx
	no equiv	all ECC HD expansions	B25CXx


XBus diagnostic control program (XCP) on disk 3 of 6 
	NGEN Modules	Description	BTOS Modules

	GC001	Graphics controller	B25GRAGRE
	GC102	Enhanced Video Controller	B39EV
	GC003	Bitmapped graphics	no equiv
	GC103	Bitmapped graphics	no equiv
	GC004	Vga+ Video Controller	B25VG3VG4
	GC104	Vga+ Video Controller	B25VG1VG2
	VC001	15 color monitor	no equiv
	VC002	15 color monitor	B25CD3
	VC003	15 Color HiRes monitor	B25CA1
	VM001	12 monochrome monitor	B25D1
	VM002	14 monochrome monitor	B25D2
	VM003	15 Mono HiRes monitor	no equiv
	VM004	15 positive polarity mon	B25PD8
	VM005	15 Mono HiRes monitor	B25GS1
	no equiv	12 positive polarity mon	B25PD7
	VA001	12 ColorMono monitor	no equiv
	TM001	Voice processor (wmodem)	no equiv
	VP002	Voice processor (wo modem)	B25TEL
	XE001	Ethernet	no equiv
	XE101	Ethernet	no equiv
	XC002	RS232 port expander	B25DCX
	XC102	RS232 port expander}	no equiv
Protected mode diagnostic control program (PCP) on disk 4 of 6
	NGEN Modules	Description	BTOS Modules

	CP002	 8 Mhz 286 processor	B28CPU
	CP002287	 8 Mhz 286 processor	B28MCP
	CP0A2	 8 Mhz 286 wEnhanced Video	B28EV
	CP0A2287	 8 Mhz 286287 wEV	B28MEV
	CP0E2	 8 Mhz 286 with EV	B28EXP
	CP003	16 Mhz 386 processor	B38CPU
	CP003287	16 Mhz 386 processor	B38MCP
	CP0A3	16 Mhz 386 wEnhanced Video	B38EV
	CP0A3287	16 Mhz 386287 wEV	B38MEV
	CM004	 8 Mhz 286 with EV	B28LCW
	no equiv	1Mb version B28EXP	B28EX1
	no equiv	1Mb version B28LCW	B28LC1
	no equiv	25 Mhz 386 wEnhanced Video	B38EXP
	no equiv	25 MHZ 386 WB25VG1	B38GXP
	PHD010	Series 286i  processor	no equiv
	PHD011	Series 286i  processor	no equiv
	PHD020	Series 286i  processor	no equiv
	PHD14x	Series 386i  processor	B3913A
	PHD32x	Series 386i  processor	B3924B
	PHD040	25MHZ  386i  processors	B395
	no equiv	12Bit Sync comm option	B25ASB
	no equiv	Hardware ID option	BxxHIAHID


SCSI diagnostic control program (SCP) on disk 5 of 6
	NGEN Modules	Description	BTOS Modules

	PHDxxx	all 386i internal SCSI HD	B39x
	HSD040	40 Mb SCSI HD wFloppy	B25MS5
	HSD020	80 Mb SCSI HD wFloppy	B25MS6
	HSX020	80 Mb SCSI HD expansion	B25XS6
	HSD140	140 Mb SCSI HD Upgrade	B25MS7
	HSX140	140 Mb SCSI HD Expansion	B25XS7
	HSD320	320 Mb SCSI HD Upgrade	B25MS8
	HSX320	320 Mb SCSI HD Expansion	B25XS8
	CD001	CDROM wController	B25CDC
	CD002	CDROM wo Controller	B25CDX
	HSB002	SCSI QIC Tape Drive	B25TS2


Coprocessor diagnostic control program (CCP) on disk 6 of 6
	NGEN Modules	Description	BTOS Modules

	PC001	PC Emulator	B251PC
	PC101	PC Emulator	no equiv
	no equiv	Smart Ethernet	B25EN3
	no equiv	ID2 Smart Comm	B25IDSID2
	no equiv	Token Ring Comm	B25TR2
