IMageDisk Analyzer 1.20 / Jan 09 2024
IMD 1.17: 24/01/1990 22:26:48

(no label)

Required cylinders: 77
Required heads    : 1
Data rate         : 500kbps
Est. maximum track: 10066 bytes

Possible drives/options to write B11D15.IMD :

 3.5" HD 80-track   NOTE: *1 *2
   Double-step: OFF

 5.25" HD 80-track   NOTE: *1
   Double-step: OFF

 8" 77-track
   Double-step: OFF

*1 77 track image likely from 8" drive.
*2 Should fit on 360rpm drive, 300rpm drive will leave long end gap.



IMageDisk Utility 1.20 / Jan 09 2024
IMD 1.17: 24/01/1990 22:26:48

(no label)

Assuming 1:1 for Binary output
 0/0 500 kbps DD  9x1024
      1   6   2   7   3   8   4   9   5  
      D   D   D   D   D   D   D   DE5 D  
 1/0  D   D   D   D   D   D   DE5 D   D  
 2/0  D   D   D   D   D   D   D   DE5 D  
 3/0  D   D   D   D   D   D   D   D   D  
 4/0  DE5 D   D   D   D   D   D   D   D  
 5/0  D   D   D   D   D   D   D   D   D  
 6/0  D   D   D   D   D   D   D   D   D  
 7/0  D   D   D   D   D   D   D   D   D  
 8/0  D   D   D   DE5 D   D   D   D   DE5
 9/0  D   D   D   D   D   DE5 DE5 D   D  
10/0  DE5 D   D   D   D   D   D   D   D  
11/0  D   D   D   D   D   D   D   D   D  
12/0  D   D   D   D   D   D   D   D   D  
13/0  D   D   D   D   D   D   D   D   D  
14/0  D   D   D   D   D   D   D   D   D  
15/0  D   D   D   D   D   D   D   D   D  
16/0  D   D   D   D   D   D   D   D   D  
17/0  D   D   D   D   D   D   D   D   D  
18/0  D   D   D   D   D   D   D   D   D  
19/0  D   D   D   D   D   D   D   D   D  
20/0  D   D   D   D   D   D   D   D   D  
21/0  D   D   D   D   D   D   DE5 D   D  
22/0  D   D   D   D   D   D   D   D   D  
23/0  D   D   D   D   D   DE5 D   D   D  
24/0  D   D   D   D   D   D   D   D   D  
25/0  D   D   D   D   D   D   D   D   D  
26/0  D   D   D   D   DE5 D   D   D   D  
27/0  D   D   D   D   D   D   D   D   D  
28/0  D   D   D   D   D   D   D   D   D  
29/0  D   D   D   D   D   D   D   D   D  
30/0  D   D   D   D   D   D   D   D   D  
31/0  D   D   D   D   D   DE5 DE5 D   D  
32/0  D   D   D   D   DE5 D   D   D   DE5
33/0  D   D   D   D   D   D   DE5 D   D  
34/0  D   D   D   D   D   D   D   D   D  
35/0  D   D   D   D   D   D   D   D   D  
36/0  D   D   D   D   D   D   D   D   D  
37/0  D   D   D   D   D   D   D   D   D  
38/0  D   D   D   D   D   D   D   D   D  
39/0  D   D   D   D   D   DE5 D   D   D  
40/0  D   D   D   D   D   D   D   DE5 D  
41/0  D   DE5 DE5 D   D   DE5 DE5 D   D  
42/0  DE5 D   D   DE5 DE5 D   D   D   DE5
43/0  D   D   D   D   D   D   D   D   D  
44/0  D   D   D   D   D   D   D   D   D  
45/0  D   D   D   D   D   D   D   D   D  
46/0  D   D   D   D   D   D   D   D   D  
47/0  D   D   D   D   D   D   D   D   D  
48/0  D   D   D   D   D   D   D   D   D  
49/0  D   D   D   D   D   D   D   D   D  
50/0  D   D   D   D   D   D   D   D   D  
51/0  D   D   D   D   D   D   D   D   D  
52/0  D   D   D   D   D   D   D   D   D  
53/0  D   D   D   D   D   D   D   D   D  
54/0  D   D   D   D   D   D   D   D   D  
55/0  D   D   D   D   D   D   D   D   D  
56/0  D   D   D   D   D   D   D   D   D  
57/0  D   D   D   D   D   D   D   D   D  
58/0  D   D   D   D   D   D   D   D   D  
59/0  D   D   D   D   D   D   D   D   D  
60/0  D   D   D   D   D   D   D   D   D  
61/0  D   D   D   D   D   D   D   D   D  
62/0  D   D   D   D   DE5 D   D   D   D  
63/0  D   D   D   D   D   D   D   D   D  
64/0  D   D   D   D   D   D   D   D   D  
65/0  D   D   D   D   D   D   D   D   D  
66/0  D00 D   D   D   D   D   D   D   D  
67/0  D   D   D   D   D   D   D   D   D  
68/0  D   D   D   D   D   D   D   D   D  
69/0  D   D   D   D   D   D   D   D   D  
70/0  DE5 D   D   DE5 D   D   D   D   D  
71/0  D   D   D   D   D   D   D   D   D  
72/0  D   D   D   D   D   D   D   D   D  
73/0  D   DE5 D   D   D   D   D   D   D  
74/0  D   D   D   D   DE5 D   D   D   D  
75/0  D   D   D   D   D   D   D   D   D  
76/0  DE5 DE5 D   DE5 DE5 DE5 DE5 DE5 DE5
77 tracks(77/0), 693 sectors (41 Compressed)



BEGIN XER5  Xerox 16/8 - SSDD 8" - 256 x 26
DENSITY MFM, HIGH
CYLINDERS 77 SIDES 1 SECTORS 26,256 SKEW 5
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20,21,22,23,24,25,26
BSH 4 BLM 15 EXM 1 DSM 242 DRM 127 AL0 0C0H AL1 0 OFS 2
END

# XER5  Xerox 16/8 - SSDD 8" - 256 x 26
diskdef xer5
  seclen 256
  tracks 77
  sectrk 26
  blocksize 2048
  maxdir 128
  skew 1
#  boottrk 2
  offset 23296
#  offset 9984
  boottrk 0
  os 2.2
end

# libdsk
[xer5]
description = XER5  Xerox 16/8 - SSDD 8" - 256 x 26
cylinders = 77
heads = 1
secsize = 256
sectors = 26
secbase = 1
datarate = ED

# Flashfloppy/GOTEK
[xer5]
cyls = 77
heads = 1
secs = 26
interleave = 1
bps = 256
id = 1
rpm = 360
#rpm = 300
rate = 250
mode = mfm
iam = no



Directory is located at 0x2400 = 9216
00002400   00 2D 53 59  53 54 45 4D  20 30 30 31  00 00 00 00  .-SYSTEM 001....
00002410   00 00 00 00  00 00 00 00  00 00 00 00  00 00 00 00  ................
00002420   00 41 53 4D  20 20 20 20  20 43 4F 4D  00 00 00 40  .ASM     COM...@
00002430   02 00 03 00  04 00 05 00  00 00 00 00  00 00 00 00  ................
00002440   00 41 53 4D  5A 20 20 20  20 43 4F 4D  00 00 00 58  .ASMZ    COM...X
00002450   06 00 07 00  08 00 09 00  0A 00 0B 00  00 00 00 00  ................
00002460   00 42 41 53  49 43 20 20  20 43 4F 4D  00 00 00 60  .BASIC   COM...`
00002470   0C 00 0D 00  0E 00 0F 00  10 00 11 00  00 00 00 00  ................
00002480   00 42 41 54  43 48 20 20  20 43 4F 4D  00 00 00 03  .BATCH   COM....
00002490   12 00 00 00  00 00 00 00  00 00 00 00  00 00 00 00  ................
000024A0   00 43 42 41  53 32 20 20  20 43 4F 4D  00 00 00 80  .CBAS2   COM....
000024B0   13 00 14 00  15 00 16 00  17 00 18 00  19 00 1A 00  ................
000024C0   00 43 42 41  53 32 20 20  20 43 4F 4D  01 00 00 1E  .CBAS2   COM....
000024D0   1B 00 1C 00  00 00 00 00  00 00 00 00  00 00 00 00  ................
000024E0   00 43 44 4F  53 44 42 55  47 43 4F 4D  00 00 00 3C  .CDOSDBUGCOM...<



$ cpmls -f xer5 -T rawob,xer5 -D B11D15.RAW
     Name    Bytes   Recs  Attr     update             create
------------ ------ ------ ---- -----------------  -----------------
@       .COM     0K      0    
APPEND  .OVR     1K      4    
CHROM   .AZM    12K     96    
COMPARE .COM     2K     10    
CONIN   .LIB     2K     11    
CONOT   .LIB     1K      2    
COPY    .COM     2K     10    
DBASE   .COM    17K    132    
DPATCH  .COM    16K    124    
DUMP80  .COM     2K     13    
EDIT    .COM     7K     51    
EXTRACT .COM     2K     12    
FERREL  .ASM    20K    155    
FERREL  .BIO    10K     76    
FIX     .COM    36K    286    
FIX     .DOC     3K     17    
FORMAT1 .COM     1K      8    
INDEX   .COM     2K     11    
INSTALL .COM     8K     63    
JOIN    .OVR     1K      2    
L80     .COM    10K     74    
LD      .COM     3K     19 R  
LOAD    .COM     2K     14    
M80     .COM    19K    150    
MAC     .COM    12K     92    
MACZ1   .COM    13K    102    
MACZLIB .REL     1K      2    
MACZLINK.COM     7K     54    
MAILMRGE.OVR     8K     60    
MAIN    .OVR     1K      5    
MAKE    .COM     1K      6    
MAST    .CAT     1K      1    
MBASIC5 .COM    24K    189    
MDIR    .COM     1K      5    
MISC    .OVR     1K      1    
MODIFY  .OVR     1K      1    
MTEST   .COM     4K     32    
MTEST1  .COM     5K     36    
MTEST2  .COM     9K     69    
MTST    .COM     1K      6    
MX80PD  .LIB     1K      6    
NSWP    .COM    11K     86 R  
READ    .ME      1K      7    
READDISK.COM     1K      6    
RPG     .OVR     1K      4    
SD      .COM     4K     30    
SEEK    .COM     1K      3    
SEEKEY  .COM     2K     16    
SH      .COM    10K     76    
SORT    .OVR     1K      4    
STAT    .COM     6K     41    
STEP0981.COM     5K     40    
STEPPER .COM     6K     46    
SURVEY  .COM     2K      9    
SYSGEN  .COM     1K      4    
TERM    .COM    12K     90    
TERM    .DEF     1K      1    
TOTAL   .OVR     1K      2    
TVC     .AZM     5K     38    
TVC     .COM     1K      7    
TVC80   .AZM    21K    164    
TVC80   .HEX     5K     38    
TVC80   .PRN    39K    310    
TVCMAN  .DOC     8K     58    
TVCMOD  .DOC     6K     48    
UMPIRE  .COM     2K     10    
UMPIRE  .DOC     2K     10    
UPDATE  .OVR     1K      7    
VERIFY  .COM     1K      3    
VMSGS$$$.COM     8K     59    
WS      .COM    16K    126    
WSH19   .COM    16K    124    
WSMSGS  .OVR    28K    218    
WSOVLY1 .OVR    34K    266    
WSTV    .COM    16K    124    
XAMN    .COM    27K    209 R  
Z80MR   .COM    14K    106    
Z80MR   .DOC    17K    134    
ZSID    .COM    10K     80    
   79 Files occupying    325K,     171K Free.


