IMageDisk Analyzer 1.20 / Jan 09 2024
IMD 1.17: 22/01/1990 22:48:49

CP/M  SS/SD

Required cylinders: 77
Required heads    : 1
Data rate         : 500kbps
Est. maximum track: 5623 bytes

Possible drives/options to write B11D8.IMD :

 3.5" HD 80-track   NOTE: *1 *2
   Double-step: OFF

 5.25" HD 80-track   NOTE: *1
   Double-step: OFF

 8" 77-track
   Double-step: OFF

*1 77 track image likely from 8" drive.
*2 Should fit on 360rpm drive, 300rpm drive will leave long end gap.



IMageDisk Utility 1.20 / Jan 09 2024
IMD 1.17: 22/01/1990 22:48:49

CP/M  SS/SD

Assuming 1:1 for Binary output
 0/0 500 kbps SD  26x128
     1  2  3  4  5  6  7  8  9  10 11 12 13 14 15 16 17 18 19 20 21 22 23 24 25 26 
     DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
 1/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
 2/0 D  DE5DE5D  DE5D  D  DE5DE5D  DE5D  D  DE5DE5D  DE5D  D  D  DE5D  DE5D  D  D  
 3/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
 4/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
 5/0 D  D  DE5D  DE5D  D  D  D  D  DE5D  D  D  D  D  DE5D  D  D  D  D  DE5D  DE5D  
 6/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
 7/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
 8/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
 9/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
10/0 D  D  D  D  D  D  D  D1AD  D  D  D  D  D1AD  D  D  D  D  D  D  D  D  D  D  D  
11/0 D  D  D00D  D00D  D  D  D  D  D  D  D  D  D00D  D00D  D  D  D  D  D00D  D  D  
12/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
13/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
14/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
15/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
16/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
17/0 D  D  D  DE5D  D  D  D  D  DE5D  D  D  D  D  DE5D  D  D  D  D  DE5D  D  D  D  
18/0 D  D  D  D  D  D00D  D  D  D  D  D00D  D00D  D  D  D  D  D  D  D  D  D00D  D00
19/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
20/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
21/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
22/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
23/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
24/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
25/0 D  D  DE5D  D  D  D  D  D  D  D  D  D  D  D  D  DE5D  D  D  D  D  DE5D  D  D  
26/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
27/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
28/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
29/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
30/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
31/0 D  DE5D  D  D  D  D  D  D  D  D  D  D  D  DE5D  D  D  D  D  DE5D  D  D  D  D  
32/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
33/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
34/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
35/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
36/0 D  D  DE5D  D  D  D  D  DE5D  D  D  D  D  DE5D  DE5D  D  D  D  D  DE5D  D  D  
37/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
38/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
39/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
40/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
41/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
42/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
43/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
44/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
45/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
46/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
47/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
48/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
49/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
50/0 D  D1AD1AD  D  D  D  D1AD1AD  D  D  D  D1AD1AD  D  D  D  D  D1AD  D  D  D  D  
51/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
52/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
53/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D1AD  D  D  D  
54/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
55/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
56/0 D  D  D  DE5D  D  D  D  D  DE5D  D  D  D  D  DE5D  DE5D1AD  D  DE5D  DE5D  D  
57/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
58/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
59/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
60/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
61/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
62/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
63/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
64/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
65/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
66/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
67/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
68/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
69/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
70/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
71/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
72/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
73/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
74/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
75/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
76/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
77 tracks(77/0), 2002 sectors (631 Compressed)



BEGIN A1  Generic CP/M - SSSD 8" - 128 x 26
DENSITY FM, HIGH
CYLINDERS 77 SIDES 1 SECTORS 26,128
SIDE1 0 1,7,13,19,25,5,11,17,23,3,9,15,21,2,8,14,20,26,6,12,18,24,4,10,16,22
BSH 3 BLM 7 EXM 0 DSM 242 DRM 63 AL0 0C0H AL1 0 OFS 2
END

# A1  Generic CP/M - SSSD 8" - 128 x 26
diskdef a1
  seclen 128
  tracks 77
  sectrk 26
  blocksize 1024
  maxdir 64
  skew 6
  boottrk 2
  os 2.2
end

# libdsk
[a1]
description = A1  Generic CP/M - SSSD 8" - 128 x 26
cylinders = 77
heads = 1
secsize = 128
sectors = 26
secbase = 1
datarate = HD

# Flashfloppy/GOTEK
[a1]
cyls = 77
heads = 1
secs = 26
interleave = 6
bps = 128
id = 1
rpm = 360
#rpm = 300
rate = 125
mode = fm
iam = no



Directory is at 0x1A00 = 6656 Decimal
00001A00   00 44 49 53  5A 49 4C 4F  47 43 4F 4D  00 00 00 42  .DISZILOGCOM...B
00001A10   02 03 04 05  06 07 08 09  0A 00 00 00  00 00 00 00  ................
00001A20   00 44 53 4B  55 54 49 4C  20 43 4F 4D  00 00 00 10  .DSKUTIL COM....
00001A30   0B 0C 00 00  00 00 00 00  00 00 00 00  00 00 00 00  ................
00001A40   00 46 4F 52  4D 41 54 31  20 43 4F 4D  00 00 00 08  .FORMAT1 COM....
00001A50   0D 00 00 00  00 00 00 00  00 00 00 00  00 00 00 00  ................
00001A60   00 46 4F 52  4D 41 54 31  20 5A 38 30  00 00 00 70  .FORMAT1 Z80...p
00001A70   0E 0F 10 11  12 13 14 15  16 17 18 19  1A 1B 00 00  ................



$ cpmls -f a1 -D B11D8.RAW
     Name    Bytes   Recs  Attr     update             create
------------ ------ ------ ---- -----------------  -----------------
DISZILOG.COM     9K     66    
DSKUTIL .COM     2K     16    
FORMAT1 .COM     1K      8    
FORMAT1 .Z80    14K    112    
MBAS501 .COM    24K    188    
MBASIC5 .COM    24K    189    
MOLD    .BAS    20K    157    
MOLD1   .BAS    16K    123    
PROM31  .MAC    46K    368    
READDISK.Z80    11K     88    
XROXGEN .ASM     7K     56    
XROXLOAD.MAC     2K     16    
   12 Files occupying    176K,      72K Free.


