IMageDisk Analyzer 1.20 / Jan 09 2024
IMD 1.17: 25/01/1990 22:04:14

E.COM??T GOOD EDITOR

Required cylinders: 77
Required heads    : 1
Data rate         : 500kbps
Est. maximum track: 5623 bytes

Possible drives/options to write B13D13.IMD :

 3.5" HD 80-track   NOTE: *1 *2
   Double-step: OFF

 5.25" HD 80-track   NOTE: *1
   Double-step: OFF

 8" 77-track
   Double-step: OFF

*1 77 track image likely from 8" drive.
*2 Should fit on 360rpm drive, 300rpm drive will leave long end gap.



IMageDisk Utility 1.20 / Jan 09 2024
IMD 1.17: 25/01/1990 22:04:14

E.COM??T GOOD EDITOR

Assuming 1:1 for Binary output
 0/0 500 kbps SD  26x128
     1  2  3  4  5  6  7  8  9  10 11 12 13 14 15 16 17 18 19 20 21 22 23 24 25 26 
     DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
 1/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
 2/0 D  DE5DE5D  DE5D  D  DE5DE5D  DE5D  D  DE5DE5D  DE5D  D  D  DE5D  DE5D  DE5D  
 3/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
 4/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
 5/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
 6/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
 7/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
 8/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
 9/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
10/0 D  D  D  DE5D  DE5D  D  D  DE5D  DE5D  D  D  D  D  DE5D  D  D  D  D  DE5D  D  
11/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
12/0 D  D  D  D  DE5D  DE5D  D  D  DE5D  DE5D  D  D  DE5D  DE5D  D  D  DE5D  DE5D  
13/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
14/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
15/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
16/0 D  D  DE5D  DE5D  D  D  DE5D  DE5D  D  D  D  D  DE5D  DE5D  D  D  DE5D  DE5D  
17/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
18/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
19/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
20/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
21/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
22/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
23/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
24/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
25/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
26/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
27/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
28/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
29/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
30/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
31/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
32/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
33/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
34/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
35/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
36/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
37/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
38/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
39/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
40/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
41/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
42/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
43/0 D  D  D00D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D00D  D  D  
44/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
45/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
46/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
47/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
48/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
49/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
50/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
51/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
52/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
53/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
54/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
55/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
56/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
57/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
58/0 D  D  D  D  D  D  D  D  D00D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
59/0 D  DE5D  DE5D00DE5D  DE5D  DE5D  DE5D  DE5D  DE5D  DE5D  DE5DE5DE5D  DE5D  DE5
60/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
61/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
62/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
63/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
64/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
65/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
66/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
67/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
68/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
69/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
70/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
71/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
72/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
73/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
74/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
75/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
76/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
77 tracks(77/0), 2002 sectors (546 Compressed)



Directory is at 0x1A00 = 6656 Decimal
00001A00   00 50 53 45  54 31 35 20  20 4C 42 52  00 00 00 80  .PSET15  LBR....
00001A10   02 03 04 05  06 07 08 09  0A 0B 0C 0D  0E 0F 10 11  ................
00001A20   00 50 53 45  54 31 35 20  20 4C 42 52  01 00 00 52  .PSET15  LBR...R
00001A30   12 13 14 15  16 17 18 19  1A 1B 1C 00  00 00 00 00  ................
00001A40   00 45 58 50  52 45 53 53  20 4C 42 52  00 00 00 80  .EXPRESS LBR....
00001A50   1D 1E 1F 20  21 22 23 24  25 26 27 28  29 2A 2B 2C  ... !"#$%&'()*+,
00001A60   00 45 58 50  52 45 53 53  20 4C 42 52  01 00 00 80  .EXPRESS LBR....
00001A70   2D 2E 2F 30  31 32 33 34  35 36 37 38  39 3A 3B 3C  -./0123456789:;<



BEGIN A1  Generic CP/M - SSSD 8" - 128 x 26
DENSITY FM, HIGH
CYLINDERS 77 SIDES 1 SECTORS 26,128
SIDE1 0 1,7,13,19,25,5,11,17,23,3,9,15,21,2,8,14,20,26,6,12,18,24,4,10,16,22
BSH 3 BLM 7 EXM 0 DSM 242 DRM 63 AL0 0C0H AL1 0 OFS 2
END

# A1  Generic CP/M - SSSD 8" - 128 x 26
diskdef a1
  seclen 128
  tracks 77
  sectrk 26
  blocksize 1024
  maxdir 64
  skew 6
  boottrk 2
  os 2.2
end

# libdsk
[a1]
description = A1  Generic CP/M - SSSD 8" - 128 x 26
cylinders = 77
heads = 1
secsize = 128
sectors = 26
secbase = 1
datarate = HD

# Flashfloppy/GOTEK
[a1]
cyls = 77
heads = 1
secs = 26
interleave = 6
bps = 128
id = 1
rpm = 360
#rpm = 300
rate = 125
mode = fm
iam = no



$ cpmls -f a1 -D B13D13.RAW
     Name    Bytes   Recs  Attr     update             create
------------ ------ ------ ---- -----------------  -----------------
EXPRESS .LBR   122K    976    
FIX     .COM    36K    286    
PSET15  .LBR    27K    210    
    3 Files occupying    185K,      63K Free.






