IMageDisk Analyzer 1.20 / Jan 09 2024
IMD 1.17:  4/02/1990 13:28:03

3780  4.2  SSSD

Required cylinders: 77
Required heads    : 1
Data rate         : 500kbps
Est. maximum track: 5623 bytes

Possible drives/options to write B4D10.IMD :

 3.5" HD 80-track   NOTE: *1 *2
   Double-step: OFF

 5.25" HD 80-track   NOTE: *1
   Double-step: OFF

 8" 77-track
   Double-step: OFF

*1 77 track image likely from 8" drive.
*2 Should fit on 360rpm drive, 300rpm drive will leave long end gap.



IMageDisk Utility 1.20 / Jan 09 2024
IMD 1.17:  4/02/1990 13:28:03

3780  4.2  SSSD

Assuming 1:1 for Binary output
 0/0 500 kbps SD  26x128
     1  2  3  4  5  6  7  8  9  10 11 12 13 14 15 16 17 18 19 20 21 22 23 24 25 26 
     DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
 1/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
 2/0 D  DE5DE5D  DE5D  D  DE5DE5D  DE5D  DE5DE5DE5D  DE5D  DE5D  DE5D  DE5D  DE5D  
 3/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
 4/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
 5/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
 6/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
 7/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
 8/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
 9/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
10/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
11/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
12/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
13/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
14/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D00
15/0 D  D  D  D  DE5D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  DE5D  
16/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
17/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
18/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
19/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
20/0 DE5D  D  D  D  D  DE5D  D  D  D  D  DE5D  D  D  D  D  DE5D  D  D  D  D  D  D  
21/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
22/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
23/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
24/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
25/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
26/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
27/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
28/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
29/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
30/0 D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  D  
31/0 D  DE5DE5DE5D  DE5D  DE5DE5DE5D  DE5D  DE5DE5DE5D  DE5D  DE5DE5DE5DE5DE5D  DE5
32/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
33/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
34/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
35/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
36/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
37/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
38/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
39/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
40/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
41/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
42/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
43/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
44/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
45/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
46/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
47/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
48/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
49/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
50/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
51/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
52/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
53/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
54/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
55/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
56/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
57/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
58/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
59/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
60/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
61/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
62/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
63/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
64/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
65/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
66/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
67/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
68/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
69/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
70/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
71/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
72/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
73/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
74/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
75/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
76/0 DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5DE5
77 tracks(77/0), 2002 sectors (1261 Compressed)



BEGIN A1  Generic CP/M - SSSD 8" - 128 x 26
DENSITY FM, HIGH
CYLINDERS 77 SIDES 1 SECTORS 26,128
SIDE1 0 1,7,13,19,25,5,11,17,23,3,9,15,21,2,8,14,20,26,6,12,18,24,4,10,16,22
BSH 3 BLM 7 EXM 0 DSM 242 DRM 63 AL0 0C0H AL1 0 OFS 2
END

# A1  Generic CP/M - SSSD 8" - 128 x 26
diskdef a1
  seclen 128
  tracks 77
  sectrk 26
  blocksize 1024
  maxdir 64
  skew 6
  boottrk 2
  os 2.2
end

# libdsk
[a1]
description = A1  Generic CP/M - SSSD 8" - 128 x 26
cylinders = 77
heads = 1
secsize = 128
sectors = 26
secbase = 1
datarate = HD

# Flashfloppy/GOTEK
[a1]
cyls = 77
heads = 1
secs = 26
interleave = 6
bps = 128
id = 1
rpm = 360
#rpm = 300
rate = 125
mode = fm
iam = no



Directory is at 0x1A00 = 6656 Decimal
00001A00   00 42 49 53  33 37 38 30  20 43 4F 4D  00 00 00 80  .BIS3780 COM....
00001A10   02 03 04 05  06 07 08 09  0A 0B 0C 0D  0E 0F 10 11  ................
00001A20   00 42 49 53  33 37 38 30  20 43 4F 4D  01 00 00 80  .BIS3780 COM....
00001A30   12 13 14 15  16 17 18 19  1A 1B 1C 1D  1E 1F 20 21  .............. !
00001A40   00 42 49 53  33 37 38 30  20 43 4F 4D  02 00 00 40  .BIS3780 COM...@
00001A50   22 23 24 25  26 27 28 29  00 00 00 00  00 00 00 00  "#$%&'()........
00001A60   00 42 49 53  33 37 38 30  43 43 4F 4D  00 00 00 06  .BIS3780CCOM....
00001A70   2A 00 00 00  00 00 00 00  00 00 00 00  00 00 00 00  *...............



$ cpmls -f a1 -D B4D10.RAW
     Name    Bytes   Recs  Attr     update             create
------------ ------ ------ ---- -----------------  -----------------
BIS3780 .COM    40K    320    
BIS3780C.COM     1K      6    
BIS3780C.MAC    16K    124    
BIS3780C.PRN    37K    290    
    4 Files occupying     94K,     154K Free.



